<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<schematic>
<libraries>
<library name="supply1">
<packages>
</packages>
<symbols>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VCC" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="VCC" symbol="VCC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="rcl">
<packages>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="L2012C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="L2825P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="L3216C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="L3225M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L3225P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="L3230M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L4035M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L4516C">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;</description>
</package>
<package name="L4532M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L4532P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="L5038P">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
precision wire wound</description>
</package>
<package name="L5650M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L8530M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="L1812">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="TJ3-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ3-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ4-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ4-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ5-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ5-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ6-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ6-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ7-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ7-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ8-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ8-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ9-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="TJ9-U2">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="POWER-CHOKE_WE-TPC">
<description>&lt;b&gt;POWER-CHOKE WE-TPC&lt;/b&gt;&lt;p&gt;
Würth Elektronik, Partnumber: 744053220&lt;br&gt;
Source: WE-TPC 744053220.pdf</description>
</package>
<package name="2200-12.7">
<description>&lt;b&gt;newport components&lt;/b&gt; 2200 Serie RM 12.7 mm&lt;p&gt;
Miniatur Axial Lead Inductors&lt;br&gt;
Source: www.rsonline.de&lt;br&gt;
Order code 240-517</description>
</package>
<package name="2200-15.24">
<description>&lt;b&gt;newport components&lt;/b&gt; 2200 Serie RM 15.24 mm&lt;p&gt;
Miniatur Axial Lead Inductors&lt;br&gt;
Source: www.rsonline.de&lt;br&gt;
Order code 240-517</description>
</package>
<package name="2200-11.43">
<description>&lt;b&gt;newport components&lt;/b&gt; 2200 Serie RM 11.43 mm&lt;p&gt;
Miniatur Axial Lead Inductors&lt;br&gt;
Source: www.rsonline.de&lt;br&gt;
Order code 240-517</description>
</package>
<package name="CEP125">
<description>&lt;b&gt;POWER INDUCTORS&lt;/b&gt; (SMT Type)&lt;p&gt;
Source: www.sumida.com/products/pdf/CEP125.pdf</description>
</package>
<package name="L0201">
<description>&lt;b&gt;NIS02 Chip Inductor&lt;/b&gt;&lt;p&gt;
Source: http://www.niccomp.com/Catalog/nis.pdf</description>
</package>
<package name="PIS2816">
<description>&lt;b&gt;PIS 2826&lt;/b&gt; Inductor&lt;p&gt;
Source: http://www.stetco.com/products/inductors/pdf/PIS2816.pdf</description>
</package>
<package name="IR-2">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. ir.pdf</description>
</package>
<package name="IR-4">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. ir.pdf</description>
</package>
<package name="IRF-1">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. irf.pdf</description>
</package>
<package name="IRF-3">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. irf.pdf</description>
</package>
<package name="IRF24">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. irf24.pdf</description>
</package>
<package name="IRF36">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. irf36.pdf</description>
</package>
<package name="IRF46">
<description>&lt;B&gt;Vishay Dale Inductor&lt;/b&gt;&lt;p&gt;
Source: www.vishay.com .. irf46.pdf</description>
</package>
<package name="LAL02">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="LAL03">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="LAL03KH">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="LAL04">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="LAL04KB">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="LAN02KR">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="LAP02KR">
<description>&lt;b&gt;TAYO YUDEN Inductor&lt;/b&gt;&lt;p&gt;
Source: je999f5.pdf</description>
</package>
<package name="TFI0204">
<description>&lt;b&gt;Axial Conformal Coated Inductor&lt;/b&gt;&lt;p&gt;
Source: TOP MAGNETICS CORPORATION .. tfi.pdf</description>
</package>
<package name="TFI0305">
<description>&lt;b&gt;Axial Conformal Coated Inductor&lt;/b&gt;&lt;p&gt;
Source: TOP MAGNETICS CORPORATION .. tfi.pdf</description>
</package>
<package name="TFI0307">
<description>&lt;b&gt;Axial Conformal Coated Inductor&lt;/b&gt;&lt;p&gt;
Source: TOP MAGNETICS CORPORATION .. tfi.pdf</description>
</package>
<package name="TFI0410">
<description>&lt;b&gt;Axial Conformal Coated Inductor&lt;/b&gt;&lt;p&gt;
Source: TOP MAGNETICS CORPORATION .. tfi.pdf</description>
</package>
<package name="TFI0510">
<description>&lt;b&gt;Axial Conformal Coated Inductor&lt;/b&gt;&lt;p&gt;
Source: TOP MAGNETICS CORPORATION .. tfi.pdf</description>
</package>
<package name="0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="6000-XXXX-RC">
<description>&lt;b&gt;Radial Lead RF Chokes&lt;/b&gt;&lt;p&gt;
Source: www.bourns.com .. 6000_series.pdf</description>
</package>
</packages>
<symbols>
<symbol name="L-EU">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="L-EU" prefix="L" uservalue="yes">
<description>&lt;B&gt;INDUCTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="L-EU"/>
</gates>
<devices>
<device name="L2012C" package="L2012C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L2825P" package="L2825P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3216C" package="L3216C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3225M" package="L3225M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3225P" package="L3225P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L3230M" package="L3230M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4035M" package="L4035M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4516C" package="L4516C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4532C" package="L4532M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L4532P" package="L4532P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L5038P" package="L5038P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L5650M" package="L5650M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L8530M" package="L8530M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204V" package="0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L1812" package="L1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ3-U1" package="TJ3-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ3-U2" package="TJ3-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ4-U1" package="TJ4-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ4-U2" package="TJ4-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ5-U1" package="TJ5-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ5-U2" package="TJ5-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ6-U1" package="TJ6-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ6-U2" package="TJ6-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ7-U1" package="TJ7-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ7-U2" package="TJ7-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ8-U1" package="TJ8-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ8-U2" package="TJ8-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ9-U1" package="TJ9-U1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TJ9-U2" package="TJ9-U2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WE-TPC" package="POWER-CHOKE_WE-TPC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2200-12.7" package="2200-12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2200-15.24" package="2200-15.24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2200-11.43" package="2200-11.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CEP125" package="CEP125">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L0201" package="L0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PIS2816" package="PIS2816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IR-2" package="IR-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IR-4" package="IR-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRF-1" package="IRF-1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRF-3" package="IRF-3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRF-24" package="IRF24">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRF-36" package="IRF36">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRF-46" package="IRF46">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAL02" package="LAL02">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAL03" package="LAL03">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAL03KB" package="LAL03KH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAL04" package="LAL04">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAL04KB" package="LAL04KB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAN02KR" package="LAN02KR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LAP02KR" package="LAP02KR">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TFI0204" package="TFI0204">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TFI0305" package="TFI0305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TFI0307" package="TFI0307">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TFI0410" package="TFI0410">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TFI0510" package="TFI0510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="6000-XXX-RC" package="6000-XXXX-RC">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Hangar">
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="TACTILE-PTH-12MM">
</package>
<package name="TACTILE-SWITCH-1101NE">
<description>Sparkfun SKU# COM-08229</description>
</package>
<package name="REED_SWITCH_PTH">
</package>
<package name="TACTILE_SWITCH_TALL">
</package>
<package name="REED_SWITCH_PLASTIC">
</package>
<package name="KSS241G">
</package>
<package name="DM3CS">
</package>
<package name="DM3AT">
</package>
<package name="TACTILE_SWITCH_SMD-2">
</package>
<package name="PINHEAD_2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="ARDUINO_WIFI_SHIELD_V018_TG_PINHEAD_2X05_127">
</package>
<package name="2X05_SMD_1.27MM">
</package>
<package name="TF-01">
</package>
</packages>
<symbols>
<symbol name="SWITCH-MOMENTARY-2">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="SDCARD">
<pin name="CS/DAT3"/>
<pin name="DI/CMD"/>
<pin name="GND"/>
<pin name="VCC"/>
<pin name="CLK"/>
<pin name="SWITCH_A"/>
<pin name="DO/DAT0"/>
<pin name="SHIELD"/>
<pin name="SWITCH_B"/>
<pin name="DAT2"/>
<pin name="DAT1"/>
</symbol>
<symbol name="PINHEAD_2X05_127">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SWITCH-MOMENTARY-2" prefix="S">
<gates>
<gate name="G$1" symbol="SWITCH-MOMENTARY-2"/>
</gates>
<devices>
<device name="PTH" package="TACTILE-PTH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="TACTILE_SWITCH_SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD-2" package="TACTILE_SWITCH_SMD-2">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="12MM" package="TACTILE-PTH-12MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD-1101NE" package="TACTILE-SWITCH-1101NE">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_REED" package="REED_SWITCH_PTH">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TACTILE_SWITCH_TALL">
<connects>
<connect gate="G$1" pin="1" pad="A2"/>
<connect gate="G$1" pin="2" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH_REED2" package="REED_SWITCH_PLASTIC">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KSS" package="KSS241G">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD_CARD_SOCKET" prefix="SD">
<description>&lt;b&gt;SD/MMC Socket&lt;/b&gt;
Media socket for SD and MMC cards. Push-push type. Model MOLEX 503182-0853</description>
<gates>
<gate name="G$1" symbol="SDCARD"/>
</gates>
<devices>
<device name="DM3CS" package="DM3CS">
<connects>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CS/DAT3" pad="2"/>
<connect gate="G$1" pin="DI/CMD" pad="3"/>
<connect gate="G$1" pin="DO/DAT0" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="9 10 12"/>
<connect gate="G$1" pin="SWITCH_A" pad="11"/>
<connect gate="G$1" pin="SWITCH_B" pad="13"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DM3AT" package="DM3AT">
<connects>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CS/DAT3" pad="2"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="DI/CMD" pad="3"/>
<connect gate="G$1" pin="DO/DAT0" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="10 12 13"/>
<connect gate="G$1" pin="SWITCH_A" pad="A"/>
<connect gate="G$1" pin="SWITCH_B" pad="B"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TF-01" package="TF-01">
<connects>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CS/DAT3" pad="2"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="DI/CMD" pad="3"/>
<connect gate="G$1" pin="DO/DAT0" pad="7"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="SHIELD" pad="9 10 11"/>
<connect gate="G$1" pin="SWITCH_A" pad="CD"/>
<connect gate="G$1" pin="SWITCH_B" pad="12"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PINHEAD_PINHD-2X5" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PINHEAD_2X05_127"/>
</gates>
<devices>
<device name="" package="PINHEAD_2X05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PASSO127" package="ARDUINO_WIFI_SHIELD_V018_TG_PINHEAD_2X05_127">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD" package="2X05_SMD_1.27MM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun">
<packages>
<package name="S2B-PH">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X02_BIG">
</package>
<package name="S2B-PH-VERTICAL">
</package>
<package name="R_SW_TH">
</package>
<package name="1X02_LOCK_LONGPADS">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X02@1">
</package>
<package name="MOLEX-1X2">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="1X02_LOCK@1">
</package>
<package name="MOLEX-1X2_LOCK">
</package>
</packages>
<symbols>
<symbol name="M02">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="M02" prefix="JP" uservalue="yes">
<description>&lt;b&gt;Header 2&lt;/b&gt;
Standard 2-pin 0.1" header. Use with straight break away headers (SKU : PRT-00116), right angle break away headers (PRT-00553), swiss pins (PRT-00743), machine pins (PRT-00117), and female headers (PRT-00115). Molex polarized connector foot print use with SKU : PRT-08233 with associated crimp pins and housings.</description>
<gates>
<gate name="G$1" symbol="M02"/>
</gates>
<devices>
<device name="PTH" package="1X02@1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR" package="MOLEX-1X2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.5MM" package="SCREWTERMINAL-3.5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-JST-2MM-SMT" package="S2B-PH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH2" package="1X02_BIG">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4UCON-15767" package="S2B-PH-VERTICAL">
<connects>
<connect gate="G$1" pin="1" pad="GND"/>
<connect gate="G$1" pin="2" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ROCKER" package="R_SW_TH">
<connects>
<connect gate="G$1" pin="1" pad="P$3"/>
<connect gate="G$1" pin="2" pad="P$4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="SCREWTERMINAL-5MM-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK" package="1X02_LOCK@1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="POLAR_LOCK" package="MOLEX-1X2_LOCK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LOCK_LONGPADS" package="1X02_LOCK_LONGPADS">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="wuerth-elektronik">
<packages>
<package name="0603">
<description>Multilayer SMD</description>
</package>
<package name="0402">
<description>Multilayer SMD</description>
</package>
<package name="0805">
<description>Multilayer SMD</description>
</package>
<package name="1206">
<description>Multilayer SMD</description>
</package>
<package name="1210">
<description>Multilayer SMD</description>
</package>
<package name="1806">
<description>Multilayer SMD</description>
</package>
<package name="1812">
<description>Multilayer SMD</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-CBF" prefix="L" uservalue="yes">
<description>SMD EMI Suppression Ferrite Beads

- excellent anti-EMI properties 
- low DCR
- impedances till 3000 ohms
- rated current up to 6 A</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_0603" package="0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0402" package="0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1210" package="1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1806" package="1806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1812" package="1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="MyPOW">
<packages>
</packages>
<symbols>
<symbol name="VUSB">
<pin name="VUSB" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="VUSB">
<gates>
<gate name="G$1" symbol="VUSB"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply2">
<packages>
</packages>
<symbols>
<symbol name="AGND">
<pin name="AGND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AGND" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AGND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="PowerTags">
<packages>
</packages>
<symbols>
<symbol name="GND-1">
<pin name="GND" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND-1"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Cristalli">
<packages>
<package name="RESONATOR_EPSON_FC_145">
</package>
</packages>
<symbols>
<symbol name="Q1-1">
<pin name="1"/>
<pin name="2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="0213_ABS07-32.768KHZ-T" prefix="Y" uservalue="yes">
<description>32,768KHz - SMD</description>
<gates>
<gate name="G$1" symbol="Q1-1"/>
</gates>
<devices>
<device name="" package="RESONATOR_EPSON_FC_145">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CASE" value=""/>
<attribute name="MONTHLY_USAGE" value="_____"/>
<attribute name="PART_NUMBER" value="ABS07-32.768KHZ-T"/>
<attribute name="PRICE" value="_____"/>
<attribute name="SUPPLIER" value="_____"/>
<attribute name="TYPE" value="Cristalli"/>
<attribute name="VALUE" value="32,768Khz_SMD"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Connector-new">
<packages>
<package name="HW4-SMD-2.0-90D">
</package>
<package name="HW4-SMD-2.0">
</package>
</packages>
<symbols>
<symbol name="GROVE-CONNECTOR-SMD">
<pin name="1" function="dotclk"/>
<pin name="2" function="dot"/>
<pin name="3" function="dot"/>
<pin name="4" function="dot"/>
<pin name="SS1"/>
<pin name="SS2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GROVE-CONNECTOR-SMD" prefix="J" uservalue="yes">
<description>4P-SMD-2.0:320110030;4P-SMD-2.0-90D:320110032</description>
<gates>
<gate name="G$1" symbol="GROVE-CONNECTOR-SMD"/>
</gates>
<devices>
<device name="'90D'" package="HW4-SMD-2.0-90D">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="SS1" pad="SS1"/>
<connect gate="G$1" pin="SS2" pad="SS2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="'DD'" package="HW4-SMD-2.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="SS1" pad="SS1"/>
<connect gate="G$1" pin="SS2" pad="SS2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="frames">
<description>&lt;b&gt;Frames for Sheet and Layout&lt;/b&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="A4L-LOC">
</symbol>
</symbols>
<devicesets>
<deviceset name="A4L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="A4L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SCK_BASE_BOARD_v1.6">
<description>Generated from &lt;b&gt;SCK_BASE_BOARD_v1.5.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="24-PIN_VQFN_THPAD">
</package>
<package name="HANGAR_C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="HANGAR_0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="HANGAR_0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="HANGAR_0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="HANGAR_0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="HANGAR_0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="HANGAR_0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="HANGAR_0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="HANGAR_0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="HANGAR_0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="HANGAR_0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="HANGAR_0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="HANGAR_0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="HANGAR_0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="HANGAR_0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="HANGAR_0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="HANGAR_0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="HANGAR_P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="HANGAR_P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="HANGAR_0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="HANGAR_0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="HANGAR_0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="HANGAR_P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="HANGAR_P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="HANGAR_0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="HANGAR_0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="HANGAR_M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="HANGAR_M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="HANGAR_M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="HANGAR_M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="HANGAR_M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="HANGAR_MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_R0201">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
</package>
<package name="HANGAR_R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="HANGAR_R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;</description>
</package>
<package name="HANGAR_R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R1218">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
</package>
<package name="HANGAR_R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R4527">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
</package>
<package name="HANGAR_R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="HANGAR_R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="HANGAR_RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="HANGAR_V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="HANGAR_V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="HANGAR_V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="HANGAR_VMTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VMTB60">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC60&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA52">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR52&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA53">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR53&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA54">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR54&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA56">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR56&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_WSC0001">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC01/2">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC0002">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC2515">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC4527">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC6927">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="WUERTH-ELEKTRONIK_0402">
<description>Multilayer SMD</description>
</package>
<package name="WUERTH-ELEKTRONIK_0603">
<description>Multilayer SMD</description>
</package>
<package name="WUERTH-ELEKTRONIK_0805">
<description>Multilayer SMD</description>
</package>
<package name="WUERTH-ELEKTRONIK_1206">
<description>Multilayer SMD</description>
</package>
<package name="WUERTH-ELEKTRONIK_1210">
<description>Multilayer SMD</description>
</package>
<package name="WUERTH-ELEKTRONIK_1806">
<description>Multilayer SMD</description>
</package>
<package name="WUERTH-ELEKTRONIK_1812">
<description>Multilayer SMD</description>
</package>
<package name="SOIC_8-208MILS">
</package>
<package name="HANGAR_ESP12-E">
</package>
<package name="DIODE_0402_R">
</package>
<package name="HANGAR_TQFP48-7X7">
</package>
<package name="HANGAR_QFN48-7X7">
</package>
<package name="DFN6_3X3MM">
</package>
<package name="HANGAR_CON2_USB_MICRO_B_AT">
</package>
<package name="NMOS_UMT3">
</package>
<package name="HANGAR_POWERPAKSC70-6L">
</package>
</packages>
<symbols>
<symbol name="BQ24259">
<pin name="VBUS"/>
<pin name="PMID"/>
<pin name="ILIM"/>
<pin name="/PG" function="dot"/>
<pin name="STAT"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="INT"/>
<pin name="/CE" function="dot"/>
<pin name="PSEL"/>
<pin name="THERMAL"/>
<pin name="SYS"/>
<pin name="TS"/>
<pin name="QON"/>
<pin name="PGND"/>
<pin name="REGN"/>
<pin name="SW"/>
<pin name="BTST"/>
<pin name="VBAT"/>
<pin name="OTG"/>
</symbol>
<symbol name="HANGAR_R-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WUERTH-ELEKTRONIK_L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="LED_LED">
<pin name="A" direction="in"/>
<pin name="K" direction="out"/>
</symbol>
<symbol name="FLASH_S25F064LABMFI013">
<pin name="WP#/IO2"/>
<pin name="SO/IO1"/>
<pin name="CS#"/>
<pin name="VSS"/>
<pin name="VCC"/>
<pin name="IO3/RESET#"/>
<pin name="SCK"/>
<pin name="SI/IO0"/>
</symbol>
<symbol name="HANGAR_L">
<pin name="1"/>
<pin name="2"/>
</symbol>
<symbol name="HANGAR_ESP8266-12E">
<pin name="ADC" direction="pas"/>
<pin name="CH_PD" direction="in"/>
<pin name="CS0" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIO0"/>
<pin name="GPIO2"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO9"/>
<pin name="GPIO10"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="GPIO14"/>
<pin name="GPIO15"/>
<pin name="GPIO16"/>
<pin name="MISO" direction="pas"/>
<pin name="MOSI"/>
<pin name="RESET" direction="in"/>
<pin name="RXD" direction="in"/>
<pin name="SCLK"/>
<pin name="TXD" direction="out"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="HANGAR_ATSAMD21">
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GNDANA" direction="pwr"/>
<pin name="PA0/XIN32/EIC/SCOM1PAD0/TC2"/>
<pin name="PA1/XOUT32/EIC/SCOM1PAD1/TC2"/>
<pin name="PA2/EIC/AIN0"/>
<pin name="PA3/EIC/REF/AIN1"/>
<pin name="PA4/EIC/REF/AIN4/SCOM0PAD0/TC0"/>
<pin name="PA5/EIC/AIN5/SCOM0PAD1/TC0"/>
<pin name="PA6/EIC/AIN6/SCOM0PAD2/TC1"/>
<pin name="PA7/EIC/AIN7/SCOM0PAD3/TC1"/>
<pin name="PA8/I2C/AIN16/SCOM2PAD0+/TC0"/>
<pin name="PA9/I2C/EIC/AIN17/SCOM2PAD1+/TC0"/>
<pin name="PA10/EIC/AIN18/SCOM2PAD2+/TC1"/>
<pin name="PA11/EIC/AIN19/SCOM2PAD3+/TC1"/>
<pin name="PA12/I2C/EIC/SCOM2PAD0+/TC2"/>
<pin name="PA13/I2C/EIC/SCOM2PAD1+/TC2"/>
<pin name="PA14/XIN/EIC/SCOM2PAD2+/TC3"/>
<pin name="PA15/XOUT/EIC/SCOM2PAD3+/TC3"/>
<pin name="PA16/I2C/EIC/SCOM1PAD0+/TC2"/>
<pin name="PA17/I2C/EIC/SCOM1PAD1+/TC2"/>
<pin name="PA18/EIC/SCOM1PAD2+/TC3"/>
<pin name="PA19/EIC/SCOM1PAD3+/TC3"/>
<pin name="PA20/EIC/SCOM5PAD2+"/>
<pin name="PA21/EIC/SCOM5PAD3+"/>
<pin name="PA22/I2C/EIC/SCOM5PAD0+/TC4"/>
<pin name="PA23/I2C/EIC/SCOM5PAD1+/TC4"/>
<pin name="PA24/EIC/SCOM3PAD2+/TC5"/>
<pin name="PA25/EIC/SCOM3PAD3+/TC5"/>
<pin name="PA27/EIC"/>
<pin name="PA28/EIC"/>
<pin name="PA30/EIC/SCOM1PAD2/TC1"/>
<pin name="PA31/EIC/SCOM1PAD3/TC1"/>
<pin name="PB2/EIC/AIN10/SCOM5PAD0"/>
<pin name="PB3/EIC/AIN11/SCOM5PAD1"/>
<pin name="PB8/EIC/AIN2/SCOM4PAD0/TC4"/>
<pin name="PB9/EIC/AIN3/SCOM4PAD1//TC4"/>
<pin name="PB10/EIC/SCOM4PAD2/TC5"/>
<pin name="PB11/EIC/SCOM4PAD3/TC5"/>
<pin name="PB22/EIC/SCOM5PAD2"/>
<pin name="PB23/EIC/SCOM5PAD3"/>
<pin name="RESETN"/>
<pin name="VDDANA" direction="pwr"/>
<pin name="VDDCORE1" direction="in"/>
<pin name="VDDIN" direction="pwr"/>
<pin name="VDDIO1" direction="pwr"/>
<pin name="VDDIO2" direction="pwr"/>
</symbol>
<symbol name="LD39200_FIXED">
<pin name="IN"/>
<pin name="EN"/>
<pin name="OUT"/>
<pin name="SENSE"/>
<pin name="PG"/>
<pin name="GND"/>
</symbol>
<symbol name="HANGAR_MYCON2_USB">
<pin name="D+"/>
<pin name="D-"/>
<pin name="GND" direction="pas"/>
<pin name="ID"/>
<pin name="SH1" direction="pas"/>
<pin name="SH2" direction="pas"/>
<pin name="SH3" direction="pas"/>
<pin name="SH4" direction="pas"/>
<pin name="SH5" direction="pas"/>
<pin name="SH6" direction="pas"/>
<pin name="SH7" direction="pas"/>
<pin name="SH8" direction="pas"/>
<pin name="SH9" direction="pas"/>
<pin name="SH10" direction="pas"/>
<pin name="SH11" direction="pas"/>
<pin name="SH12" direction="pas"/>
<pin name="SH13" direction="pas"/>
<pin name="SH14" direction="pas"/>
<pin name="VBUS" direction="pwr"/>
</symbol>
<symbol name="NMOS">
<pin name="D" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PMOS">
<pin name="S" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BQ24259_VQFN(24)">
<gates>
<gate name="G$1" symbol="BQ24259"/>
</gates>
<devices>
<device name="" package="24-PIN_VQFN_THPAD">
<connects>
<connect gate="G$1" pin="/CE" pad="9"/>
<connect gate="G$1" pin="/PG" pad="3"/>
<connect gate="G$1" pin="BTST" pad="21"/>
<connect gate="G$1" pin="ILIM" pad="10"/>
<connect gate="G$1" pin="INT" pad="7"/>
<connect gate="G$1" pin="OTG" pad="8"/>
<connect gate="G$1" pin="PGND" pad="17 18"/>
<connect gate="G$1" pin="PMID" pad="23"/>
<connect gate="G$1" pin="PSEL" pad="2"/>
<connect gate="G$1" pin="QON" pad="12"/>
<connect gate="G$1" pin="REGN" pad="22"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="STAT" pad="4"/>
<connect gate="G$1" pin="SW" pad="19 20"/>
<connect gate="G$1" pin="SYS" pad="15 16"/>
<connect gate="G$1" pin="THERMAL" pad="25"/>
<connect gate="G$1" pin="TS" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="13 14"/>
<connect gate="G$1" pin="VBUS" pad="1 24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HANGAR_R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="HANGAR_R-EU"/>
</gates>
<devices>
<device name="0204/2V" package="HANGAR_0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="HANGAR_0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="HANGAR_0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="HANGAR_0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="HANGAR_0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="HANGAR_0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="HANGAR_0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="HANGAR_0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="HANGAR_0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="HANGAR_0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="HANGAR_0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="HANGAR_0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="HANGAR_0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="HANGAR_0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="HANGAR_0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="HANGAR_0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="HANGAR_0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="HANGAR_P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="HANGAR_P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="HANGAR_0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="HANGAR_0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="HANGAR_0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="HANGAR_P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="HANGAR_P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="HANGAR_0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="HANGAR_0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="HANGAR_M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="HANGAR_M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="HANGAR_M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="HANGAR_M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="HANGAR_M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="HANGAR_M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="HANGAR_M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="HANGAR_M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="HANGAR_MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="HANGAR_MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="HANGAR_MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="HANGAR_MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="HANGAR_MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="HANGAR_MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="HANGAR_MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0201" package="HANGAR_R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0402" package="HANGAR_R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="HANGAR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="HANGAR_R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="HANGAR_R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="HANGAR_R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="HANGAR_R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="HANGAR_R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="HANGAR_R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="HANGAR_R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1218" package="HANGAR_R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="HANGAR_R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="HANGAR_R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="HANGAR_R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="HANGAR_R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="HANGAR_R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="HANGAR_R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="HANGAR_R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="HANGAR_R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="HANGAR_R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="HANGAR_R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R4527" package="HANGAR_R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="HANGAR_R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="HANGAR_R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="HANGAR_R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="HANGAR_R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="HANGAR_RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="HANGAR_V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="HANGAR_V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="HANGAR_V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTA55" package="HANGAR_VMTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTB60" package="HANGAR_VMTB60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA52" package="HANGAR_VTA52">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA53" package="HANGAR_VTA53">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA54" package="HANGAR_VTA54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA55" package="HANGAR_VTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA56" package="HANGAR_VTA56">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0001" package="HANGAR_WSC0001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC01/2" package="HANGAR_WSC01/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0002" package="HANGAR_WSC0002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC2515" package="HANGAR_WSC2515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC4527" package="HANGAR_WSC4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC6927" package="HANGAR_WSC6927">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WUERTH-ELEKTRONIK_WE-CBF" prefix="L" uservalue="yes">
<description>SMD EMI Suppression Ferrite Beads

- excellent anti-EMI properties 
- low DCR
- impedances till 3000 ohms
- rated current up to 6 A</description>
<gates>
<gate name="G$1" symbol="WUERTH-ELEKTRONIK_L"/>
</gates>
<devices>
<device name="_0402" package="WUERTH-ELEKTRONIK_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0603" package="WUERTH-ELEKTRONIK_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_0805" package="WUERTH-ELEKTRONIK_0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1206" package="WUERTH-ELEKTRONIK_1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1210" package="WUERTH-ELEKTRONIK_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1806" package="WUERTH-ELEKTRONIK_1806">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_1812" package="WUERTH-ELEKTRONIK_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FLASH_S25FL064L">
<gates>
<gate name="G$1" symbol="FLASH_S25F064LABMFI013"/>
</gates>
<devices>
<device name="" package="SOIC_8-208MILS">
<connects>
<connect gate="G$1" pin="CS#" pad="1"/>
<connect gate="G$1" pin="IO3/RESET#" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI/IO0" pad="5"/>
<connect gate="G$1" pin="SO/IO1" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="WP#/IO2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LQH32PN1R0NNCL" uservalue="yes">
<gates>
<gate name="G$1" symbol="HANGAR_L"/>
</gates>
<devices>
<device name="" package="HANGAR_C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HANGAR_ESP-12-E" prefix="W">
<gates>
<gate name="G$1" symbol="HANGAR_ESP8266-12E"/>
</gates>
<devices>
<device name="" package="HANGAR_ESP12-E">
<connects>
<connect gate="G$1" pin="ADC" pad="2"/>
<connect gate="G$1" pin="CH_PD" pad="3"/>
<connect gate="G$1" pin="CS0" pad="9"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="GPIO0" pad="18"/>
<connect gate="G$1" pin="GPIO10" pad="12"/>
<connect gate="G$1" pin="GPIO12" pad="6"/>
<connect gate="G$1" pin="GPIO13" pad="7"/>
<connect gate="G$1" pin="GPIO14" pad="5"/>
<connect gate="G$1" pin="GPIO15" pad="16"/>
<connect gate="G$1" pin="GPIO16" pad="4"/>
<connect gate="G$1" pin="GPIO2" pad="17"/>
<connect gate="G$1" pin="GPIO4" pad="20"/>
<connect gate="G$1" pin="GPIO5" pad="19"/>
<connect gate="G$1" pin="GPIO9" pad="11"/>
<connect gate="G$1" pin="MISO" pad="10"/>
<connect gate="G$1" pin="MOSI" pad="13"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="RXD" pad="21"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="TXD" pad="22"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_SMALL" prefix="LED" uservalue="yes">
<gates>
<gate name="G$1" symbol="LED_LED"/>
</gates>
<devices>
<device name="" package="DIODE_0402_R">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="K" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HANGAR_SAMD21G18A-" prefix="IC">
<description>Atmel D21 32bit ARM Cortex-M0  microcontroller - 48 PIN TQFP
256KB flash memory + 32KB SRAM</description>
<gates>
<gate name="G$1" symbol="HANGAR_ATSAMD21"/>
</gates>
<devices>
<device name="AUT" package="HANGAR_TQFP48-7X7">
<connects>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="35"/>
<connect gate="G$1" pin="GND3" pad="42"/>
<connect gate="G$1" pin="GNDANA" pad="5"/>
<connect gate="G$1" pin="PA0/XIN32/EIC/SCOM1PAD0/TC2" pad="1"/>
<connect gate="G$1" pin="PA1/XOUT32/EIC/SCOM1PAD1/TC2" pad="2"/>
<connect gate="G$1" pin="PA10/EIC/AIN18/SCOM2PAD2+/TC1" pad="15"/>
<connect gate="G$1" pin="PA11/EIC/AIN19/SCOM2PAD3+/TC1" pad="16"/>
<connect gate="G$1" pin="PA12/I2C/EIC/SCOM2PAD0+/TC2" pad="21"/>
<connect gate="G$1" pin="PA13/I2C/EIC/SCOM2PAD1+/TC2" pad="22"/>
<connect gate="G$1" pin="PA14/XIN/EIC/SCOM2PAD2+/TC3" pad="23"/>
<connect gate="G$1" pin="PA15/XOUT/EIC/SCOM2PAD3+/TC3" pad="24"/>
<connect gate="G$1" pin="PA16/I2C/EIC/SCOM1PAD0+/TC2" pad="25"/>
<connect gate="G$1" pin="PA17/I2C/EIC/SCOM1PAD1+/TC2" pad="26"/>
<connect gate="G$1" pin="PA18/EIC/SCOM1PAD2+/TC3" pad="27"/>
<connect gate="G$1" pin="PA19/EIC/SCOM1PAD3+/TC3" pad="28"/>
<connect gate="G$1" pin="PA2/EIC/AIN0" pad="3"/>
<connect gate="G$1" pin="PA20/EIC/SCOM5PAD2+" pad="29"/>
<connect gate="G$1" pin="PA21/EIC/SCOM5PAD3+" pad="30"/>
<connect gate="G$1" pin="PA22/I2C/EIC/SCOM5PAD0+/TC4" pad="31"/>
<connect gate="G$1" pin="PA23/I2C/EIC/SCOM5PAD1+/TC4" pad="32"/>
<connect gate="G$1" pin="PA24/EIC/SCOM3PAD2+/TC5" pad="33"/>
<connect gate="G$1" pin="PA25/EIC/SCOM3PAD3+/TC5" pad="34"/>
<connect gate="G$1" pin="PA27/EIC" pad="39"/>
<connect gate="G$1" pin="PA28/EIC" pad="41"/>
<connect gate="G$1" pin="PA3/EIC/REF/AIN1" pad="4"/>
<connect gate="G$1" pin="PA30/EIC/SCOM1PAD2/TC1" pad="45"/>
<connect gate="G$1" pin="PA31/EIC/SCOM1PAD3/TC1" pad="46"/>
<connect gate="G$1" pin="PA4/EIC/REF/AIN4/SCOM0PAD0/TC0" pad="9"/>
<connect gate="G$1" pin="PA5/EIC/AIN5/SCOM0PAD1/TC0" pad="10"/>
<connect gate="G$1" pin="PA6/EIC/AIN6/SCOM0PAD2/TC1" pad="11"/>
<connect gate="G$1" pin="PA7/EIC/AIN7/SCOM0PAD3/TC1" pad="12"/>
<connect gate="G$1" pin="PA8/I2C/AIN16/SCOM2PAD0+/TC0" pad="13"/>
<connect gate="G$1" pin="PA9/I2C/EIC/AIN17/SCOM2PAD1+/TC0" pad="14"/>
<connect gate="G$1" pin="PB10/EIC/SCOM4PAD2/TC5" pad="19"/>
<connect gate="G$1" pin="PB11/EIC/SCOM4PAD3/TC5" pad="20"/>
<connect gate="G$1" pin="PB2/EIC/AIN10/SCOM5PAD0" pad="47"/>
<connect gate="G$1" pin="PB22/EIC/SCOM5PAD2" pad="37"/>
<connect gate="G$1" pin="PB23/EIC/SCOM5PAD3" pad="38"/>
<connect gate="G$1" pin="PB3/EIC/AIN11/SCOM5PAD1" pad="48"/>
<connect gate="G$1" pin="PB8/EIC/AIN2/SCOM4PAD0/TC4" pad="7"/>
<connect gate="G$1" pin="PB9/EIC/AIN3/SCOM4PAD1//TC4" pad="8"/>
<connect gate="G$1" pin="RESETN" pad="40"/>
<connect gate="G$1" pin="VDDANA" pad="6"/>
<connect gate="G$1" pin="VDDCORE1" pad="43"/>
<connect gate="G$1" pin="VDDIN" pad="44"/>
<connect gate="G$1" pin="VDDIO1" pad="17"/>
<connect gate="G$1" pin="VDDIO2" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value="SAMD21G18A-AUT"/>
</technology>
</technologies>
</device>
<device name="MUT" package="HANGAR_QFN48-7X7">
<connects>
<connect gate="G$1" pin="GND1" pad="18 TP"/>
<connect gate="G$1" pin="GND2" pad="35"/>
<connect gate="G$1" pin="GND3" pad="42"/>
<connect gate="G$1" pin="GNDANA" pad="5"/>
<connect gate="G$1" pin="PA0/XIN32/EIC/SCOM1PAD0/TC2" pad="1"/>
<connect gate="G$1" pin="PA1/XOUT32/EIC/SCOM1PAD1/TC2" pad="2"/>
<connect gate="G$1" pin="PA10/EIC/AIN18/SCOM2PAD2+/TC1" pad="15"/>
<connect gate="G$1" pin="PA11/EIC/AIN19/SCOM2PAD3+/TC1" pad="16"/>
<connect gate="G$1" pin="PA12/I2C/EIC/SCOM2PAD0+/TC2" pad="21"/>
<connect gate="G$1" pin="PA13/I2C/EIC/SCOM2PAD1+/TC2" pad="22"/>
<connect gate="G$1" pin="PA14/XIN/EIC/SCOM2PAD2+/TC3" pad="23"/>
<connect gate="G$1" pin="PA15/XOUT/EIC/SCOM2PAD3+/TC3" pad="24"/>
<connect gate="G$1" pin="PA16/I2C/EIC/SCOM1PAD0+/TC2" pad="25"/>
<connect gate="G$1" pin="PA17/I2C/EIC/SCOM1PAD1+/TC2" pad="26"/>
<connect gate="G$1" pin="PA18/EIC/SCOM1PAD2+/TC3" pad="27"/>
<connect gate="G$1" pin="PA19/EIC/SCOM1PAD3+/TC3" pad="28"/>
<connect gate="G$1" pin="PA2/EIC/AIN0" pad="3"/>
<connect gate="G$1" pin="PA20/EIC/SCOM5PAD2+" pad="29"/>
<connect gate="G$1" pin="PA21/EIC/SCOM5PAD3+" pad="30"/>
<connect gate="G$1" pin="PA22/I2C/EIC/SCOM5PAD0+/TC4" pad="31"/>
<connect gate="G$1" pin="PA23/I2C/EIC/SCOM5PAD1+/TC4" pad="32"/>
<connect gate="G$1" pin="PA24/EIC/SCOM3PAD2+/TC5" pad="33"/>
<connect gate="G$1" pin="PA25/EIC/SCOM3PAD3+/TC5" pad="34"/>
<connect gate="G$1" pin="PA27/EIC" pad="39"/>
<connect gate="G$1" pin="PA28/EIC" pad="41"/>
<connect gate="G$1" pin="PA3/EIC/REF/AIN1" pad="4"/>
<connect gate="G$1" pin="PA30/EIC/SCOM1PAD2/TC1" pad="45"/>
<connect gate="G$1" pin="PA31/EIC/SCOM1PAD3/TC1" pad="46"/>
<connect gate="G$1" pin="PA4/EIC/REF/AIN4/SCOM0PAD0/TC0" pad="9"/>
<connect gate="G$1" pin="PA5/EIC/AIN5/SCOM0PAD1/TC0" pad="10"/>
<connect gate="G$1" pin="PA6/EIC/AIN6/SCOM0PAD2/TC1" pad="11"/>
<connect gate="G$1" pin="PA7/EIC/AIN7/SCOM0PAD3/TC1" pad="12"/>
<connect gate="G$1" pin="PA8/I2C/AIN16/SCOM2PAD0+/TC0" pad="13"/>
<connect gate="G$1" pin="PA9/I2C/EIC/AIN17/SCOM2PAD1+/TC0" pad="14"/>
<connect gate="G$1" pin="PB10/EIC/SCOM4PAD2/TC5" pad="19"/>
<connect gate="G$1" pin="PB11/EIC/SCOM4PAD3/TC5" pad="20"/>
<connect gate="G$1" pin="PB2/EIC/AIN10/SCOM5PAD0" pad="47"/>
<connect gate="G$1" pin="PB22/EIC/SCOM5PAD2" pad="37"/>
<connect gate="G$1" pin="PB23/EIC/SCOM5PAD3" pad="38"/>
<connect gate="G$1" pin="PB3/EIC/AIN11/SCOM5PAD1" pad="48"/>
<connect gate="G$1" pin="PB8/EIC/AIN2/SCOM4PAD0/TC4" pad="7"/>
<connect gate="G$1" pin="PB9/EIC/AIN3/SCOM4PAD1//TC4" pad="8"/>
<connect gate="G$1" pin="RESETN" pad="40"/>
<connect gate="G$1" pin="VDDANA" pad="6"/>
<connect gate="G$1" pin="VDDCORE1" pad="43"/>
<connect gate="G$1" pin="VDDIN" pad="44"/>
<connect gate="G$1" pin="VDDIO1" pad="17"/>
<connect gate="G$1" pin="VDDIO2" pad="36"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD39200" prefix="LDO">
<gates>
<gate name="G$1" symbol="LD39200_FIXED"/>
</gates>
<devices>
<device name="" package="DFN6_3X3MM">
<connects>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="GND" pad="3 7"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="PG" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HANGAR_MYCON2_USB-MINI-B" prefix="J">
<gates>
<gate name="G$1" symbol="HANGAR_MYCON2_USB"/>
</gates>
<devices>
<device name="" package="HANGAR_CON2_USB_MICRO_B_AT">
<connects>
<connect gate="G$1" pin="D+" pad="P3"/>
<connect gate="G$1" pin="D-" pad="P2"/>
<connect gate="G$1" pin="GND" pad="P5"/>
<connect gate="G$1" pin="ID" pad="P4"/>
<connect gate="G$1" pin="SH1" pad="S1"/>
<connect gate="G$1" pin="SH10" pad="P$4"/>
<connect gate="G$1" pin="SH11" pad="P$5"/>
<connect gate="G$1" pin="SH12" pad="P$6"/>
<connect gate="G$1" pin="SH13" pad="P$7"/>
<connect gate="G$1" pin="SH14" pad="P$8"/>
<connect gate="G$1" pin="SH2" pad="S2"/>
<connect gate="G$1" pin="SH3" pad="S3"/>
<connect gate="G$1" pin="SH4" pad="S4"/>
<connect gate="G$1" pin="SH5" pad="S5"/>
<connect gate="G$1" pin="SH6" pad="S6"/>
<connect gate="G$1" pin="SH7" pad="P$1"/>
<connect gate="G$1" pin="SH8" pad="P$2"/>
<connect gate="G$1" pin="SH9" pad="P$3"/>
<connect gate="G$1" pin="VBUS" pad="P1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NMOS_RJU003N03FRAT106" prefix="NMOS">
<gates>
<gate name="G$1" symbol="NMOS"/>
</gates>
<devices>
<device name="" package="NMOS_UMT3">
<connects>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOSFETP_BOTH" uservalue="yes">
<gates>
<gate name="G$1" symbol="PMOS"/>
<gate name="G$2" symbol="PMOS"/>
</gates>
<devices>
<device name="" package="HANGAR_POWERPAKSC70-6L">
<connects>
<connect gate="G$1" pin="D" pad="6 TP1"/>
<connect gate="G$1" pin="G" pad="2"/>
<connect gate="G$1" pin="S" pad="1"/>
<connect gate="G$2" pin="D" pad="3 TP2"/>
<connect gate="G$2" pin="G" pad="5"/>
<connect gate="G$2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SCK_URBAN_SHIELD_v1.6">
<description>Generated from &lt;b&gt;SCK_URBAN_SHIELD_v1.5.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="BGA-9">
</package>
<package name="HANGAR_0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
<package name="HANGAR_0204/5">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 5 mm</description>
</package>
<package name="HANGAR_0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="HANGAR_0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="HANGAR_0207/5V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 5 mm</description>
</package>
<package name="HANGAR_0207/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="HANGAR_0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="HANGAR_0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
<package name="HANGAR_0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="HANGAR_0309/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 10mm</description>
</package>
<package name="HANGAR_0309/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 12.5 mm</description>
</package>
<package name="HANGAR_0309V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0309, grid 2.5 mm</description>
</package>
<package name="HANGAR_0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
<package name="HANGAR_0411/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 12.5 mm</description>
</package>
<package name="HANGAR_0411/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 15 mm</description>
</package>
<package name="HANGAR_0414V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 5 mm</description>
</package>
<package name="HANGAR_0414/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0414, grid 15 mm</description>
</package>
<package name="HANGAR_P0613V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 5 mm</description>
</package>
<package name="HANGAR_P0613/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0613, grid 15 mm</description>
</package>
<package name="HANGAR_0617V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 5 mm</description>
</package>
<package name="HANGAR_0617/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 17.5 mm</description>
</package>
<package name="HANGAR_0617/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0617, grid 22.5 mm</description>
</package>
<package name="HANGAR_P0817V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 6.35 mm</description>
</package>
<package name="HANGAR_P0817/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0817, grid 22.5 mm</description>
</package>
<package name="HANGAR_0922/22">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 22.5 mm</description>
</package>
<package name="HANGAR_0922V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0922, grid 7.5 mm</description>
</package>
<package name="HANGAR_M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="HANGAR_M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_M1406">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="HANGAR_M2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="HANGAR_M2309">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_M3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_M3516">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.12 W</description>
</package>
<package name="HANGAR_M5923">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="HANGAR_MINI_MELF-0102AX">
<description>&lt;b&gt;Mini MELF 0102 Axial&lt;/b&gt;</description>
</package>
<package name="HANGAR_MINI_MELF-0102R">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0102W">
<description>&lt;b&gt;CECC Size RC2211&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0204R">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0204W">
<description>&lt;b&gt;CECC Size RC3715&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0207R">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Reflow Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_MINI_MELF-0207W">
<description>&lt;b&gt;CECC Size RC6123&lt;/b&gt; Wave Soldering&lt;p&gt;
source Beyschlag</description>
</package>
<package name="HANGAR_R0201">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; chip&lt;p&gt;
Source: http://www.vishay.com/docs/20008/dcrcw.pdf</description>
</package>
<package name="HANGAR_R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="HANGAR_R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;</description>
</package>
<package name="HANGAR_R1005">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R1206W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R1210W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R1218">
<description>&lt;b&gt;CRCW1218 Thick Film, Rectangular Chip Resistors&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com .. dcrcw.pdf</description>
</package>
<package name="HANGAR_R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R2010W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R2012">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R2012W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R2512">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R2512W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R3216W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R3225">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R3225W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R4527">
<description>&lt;b&gt;Package 4527&lt;/b&gt;&lt;p&gt;
Source: http://www.vishay.com/docs/31059/wsrhigh.pdf</description>
</package>
<package name="HANGAR_R5025">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="HANGAR_R5025W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
wave soldering</description>
</package>
<package name="HANGAR_R6332">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="HANGAR_R6332W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt; wave soldering&lt;p&gt;
Source: http://download.siliconexpert.com/pdfs/2005/02/24/Semi_Ap/2/VSH/Resistor/dcrcwfre.pdf</description>
</package>
<package name="HANGAR_RDH/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type RDH, grid 15 mm</description>
</package>
<package name="HANGAR_V234/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V234, grid 12.5 mm</description>
</package>
<package name="HANGAR_V235/17">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V235, grid 17.78 mm</description>
</package>
<package name="HANGAR_V526-0">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type V526-0, grid 2.5 mm</description>
</package>
<package name="HANGAR_VMTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VMTB60">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RNC60&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA52">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR52&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA53">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR53&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA54">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR54&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA55">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR55&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_VTA56">
<description>&lt;b&gt;Bulk Metal® Foil Technology&lt;/b&gt;, Tubular Axial Lead Resistors, Meets or Exceeds MIL-R-39005 Requirements&lt;p&gt;
MIL SIZE RBR56&lt;br&gt;
Source: VISHAY .. vta56.pdf</description>
</package>
<package name="HANGAR_WSC0001">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC01/2">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC0002">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC2515">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC4527">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
<package name="HANGAR_WSC6927">
<description>&lt;b&gt;Wirewound Resistors, Precision Power&lt;/b&gt;&lt;p&gt;
Source: VISHAY wscwsn.pdf</description>
</package>
</packages>
<symbols>
<symbol name="BQ27246YZFR">
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="GPUOT"/>
<pin name="SRN"/>
<pin name="SRP"/>
<pin name="VSS"/>
<pin name="VDD"/>
<pin name="BIN"/>
<pin name="BAT"/>
</symbol>
<symbol name="HANGAR_R-EU">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="GAUGE_BQ2746">
<gates>
<gate name="BQ27426" symbol="BQ27246YZFR"/>
</gates>
<devices>
<device name="" package="BGA-9">
<connects>
<connect gate="BQ27426" pin="BAT" pad="C3"/>
<connect gate="BQ27426" pin="BIN" pad="B1"/>
<connect gate="BQ27426" pin="GPUOT" pad="A1"/>
<connect gate="BQ27426" pin="SCL" pad="A3"/>
<connect gate="BQ27426" pin="SDA" pad="A2"/>
<connect gate="BQ27426" pin="SRN" pad="C2"/>
<connect gate="BQ27426" pin="SRP" pad="C1"/>
<connect gate="BQ27426" pin="VDD" pad="B3"/>
<connect gate="BQ27426" pin="VSS" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HANGAR_R-EU_" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, European symbol</description>
<gates>
<gate name="G$1" symbol="HANGAR_R-EU"/>
</gates>
<devices>
<device name="0204/2V" package="HANGAR_0204V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/5" package="HANGAR_0204/5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0204/7" package="HANGAR_0204/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/2V" package="HANGAR_0207/2V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/5V" package="HANGAR_0207/5V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/7" package="HANGAR_0207/7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/10" package="HANGAR_0207/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/12" package="HANGAR_0207/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0207/15" package="HANGAR_0207/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/10" package="HANGAR_0309/10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/12" package="HANGAR_0309/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0309/V" package="HANGAR_0309V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/3V" package="HANGAR_0411V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/12" package="HANGAR_0411/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0411/15" package="HANGAR_0411/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/5V" package="HANGAR_0414V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0414/15" package="HANGAR_0414/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/5V" package="HANGAR_P0613V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0613/15" package="HANGAR_P0613/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/5V" package="HANGAR_0617V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/17" package="HANGAR_0617/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0617/22" package="HANGAR_0617/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/7V" package="HANGAR_P0817V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0817/22" package="HANGAR_P0817/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922/22" package="HANGAR_0922/22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0922V" package="HANGAR_0922V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M0805" package="HANGAR_M0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1206" package="HANGAR_M1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M1406" package="HANGAR_M1406">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2012" package="HANGAR_M2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M2309" package="HANGAR_M2309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3216" package="HANGAR_M3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M3516" package="HANGAR_M3516">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M5923" package="HANGAR_M5923">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102AX" package="HANGAR_MINI_MELF-0102AX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102R" package="HANGAR_MINI_MELF-0102R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0102W" package="HANGAR_MINI_MELF-0102W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204R" package="HANGAR_MINI_MELF-0204R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0204W" package="HANGAR_MINI_MELF-0204W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207R" package="HANGAR_MINI_MELF-0207R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MELF0207W" package="HANGAR_MINI_MELF-0207W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0201" package="HANGAR_R0201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0402" package="HANGAR_R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0603" package="HANGAR_R0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805" package="HANGAR_R0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R0805W" package="HANGAR_R0805W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1005" package="HANGAR_R1005">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206" package="HANGAR_R1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1206W" package="HANGAR_R1206W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210" package="HANGAR_R1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1210W" package="HANGAR_R1210W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R1218" package="HANGAR_R1218">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010" package="HANGAR_R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2010W" package="HANGAR_R2010W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012" package="HANGAR_R2012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2012W" package="HANGAR_R2012W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512" package="HANGAR_R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R2512W" package="HANGAR_R2512W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216" package="HANGAR_R3216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3216W" package="HANGAR_R3216W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225" package="HANGAR_R3225">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R3225W" package="HANGAR_R3225W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R4527" package="HANGAR_R4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025" package="HANGAR_R5025">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R5025W" package="HANGAR_R5025W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332" package="HANGAR_R6332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R6332W" package="HANGAR_R6332W">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RDH/15" package="HANGAR_RDH/15">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V234/12" package="HANGAR_V234/12">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V235/17" package="HANGAR_V235/17">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="V526-0" package="HANGAR_V526-0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTA55" package="HANGAR_VMTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VMTB60" package="HANGAR_VMTB60">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA52" package="HANGAR_VTA52">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA53" package="HANGAR_VTA53">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA54" package="HANGAR_VTA54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA55" package="HANGAR_VTA55">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="VTA56" package="HANGAR_VTA56">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0001" package="HANGAR_WSC0001">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC01/2" package="HANGAR_WSC01/2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC0002" package="HANGAR_WSC0002">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC2515" package="HANGAR_WSC2515">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC4527" package="HANGAR_WSC4527">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="WSC6927" package="HANGAR_WSC6927">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-OPL-Capacitor">
<packages>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="C1206">
</package>
<package name="C1210">
</package>
<package name="C0603">
<description>&lt;b&gt;0603&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="C">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CERAMIC-100NF-50V-10%-X7R(0805)" prefix="C" uservalue="yes">
<description>302010165</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
<attribute name="VALUE" value="100nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-10UF-25V-10%-X5R(1206)" prefix="C" uservalue="yes">
<description>302010181</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC1206KKX5R8BB106"/>
<attribute name="VALUE" value="10uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-1UF-25V-10%-X7R(0805)" prefix="C" uservalue="yes">
<description>302010179</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0805KKX7R8BB105"/>
<attribute name="VALUE" value="1uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-47UF-10V-20%-X7R(1210)" prefix="C" uservalue="yes">
<description>302010252</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="GRM32ER71A476ME15L"/>
<attribute name="VALUE" value="47uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-100NF-50V-10%-X7R(0603)" prefix="C" uservalue="yes">
<description>302010138</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX7R9BB104"/>
<attribute name="VALUE" value="100nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-4.7UF-10V-10%-X5R(0603)" prefix="C" uservalue="yes">
<description>302010111</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX5R6BB475"/>
<attribute name="VALUE" value="4.7uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-4.7UF-25V-10%-X5R(0805)" prefix="C" uservalue="yes">
<description>302010146</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0805KKX5R8BB475"/>
<attribute name="VALUE" value="4.7uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-47NF-25V-10%-X7R(0402)" prefix="C" uservalue="yes">
<description>302010002</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402KRX7R8BB473"/>
<attribute name="VALUE" value="47nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-10UF-10V-10%-X5R(0603)" prefix="C" uservalue="yes">
<description>302010103</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX5R6BB106"/>
<attribute name="VALUE" value="10uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-2.2UF-10V-10%-X7R(0603)" prefix="C" uservalue="yes">
<description>302010054</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0603KRX7R6BB225"/>
<attribute name="VALUE" value="2.2uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-22PF-50V-5%-NPO(0402)" prefix="C" uservalue="yes">
<description>302010018</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402JRNPO9BN220"/>
<attribute name="VALUE" value="22pf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-100NF-25V-10%-X7R(0402)" prefix="C" uservalue="yes">
<description>302010024</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
<attribute name="VALUE" value="100nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-1UF-10V-10%-X5R(0402)" prefix="C" uservalue="yes">
<description>302010040</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402KRX5R6BB105"/>
<attribute name="VALUE" value="1uf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CERAMIC-10NF-50V-10%-X7R(0402)" prefix="C" uservalue="yes">
<description>302010006</description>
<gates>
<gate name="G$1" symbol="C"/>
</gates>
<devices>
<device name="" package="C0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="CC0402KRX7R9BB103"/>
<attribute name="VALUE" value="10nf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-OPL-Resistor">
<packages>
<package name="R0402">
</package>
</packages>
<symbols>
<symbol name="RES">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMD-RES-10K-1%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010047</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402FR-0710KL"/>
<attribute name="VALUE" value="10K 1/16W"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-100K-5%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010033</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-07100KL"/>
<attribute name="VALUE" value="100K 1/16W"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-47K-5%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010005</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-0747KL"/>
<attribute name="VALUE" value="47K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-68K-50V-5%(0402)" prefix="R" uservalue="yes">
<description>301010496</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-0768KL"/>
<attribute name="VALUE" value="68K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-330R-1%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010466</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402FR-07330RL"/>
<attribute name="VALUE" value="330R"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-1K-5%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010006</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-071KL"/>
<attribute name="VALUE" value="1K"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="fabhack">
<packages>
<package name="DRY6">
</package>
</packages>
<symbols>
<symbol name="TPD4S012_DRY_6">
<pin name="D+" direction="pas"/>
<pin name="D-" direction="pas"/>
<pin name="ID" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="N.C." direction="pas"/>
<pin name="VBUS" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TPD4S012_DRY_6" prefix="U">
<gates>
<gate name="A" symbol="TPD4S012_DRY_6"/>
</gates>
<devices>
<device name="" package="DRY6">
<connects>
<connect gate="A" pin="D+" pad="1"/>
<connect gate="A" pin="D-" pad="2"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="ID" pad="3"/>
<connect gate="A" pin="N.C." pad="5"/>
<connect gate="A" pin="VBUS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-Resistor">
<packages>
<package name="R0402">
</package>
</packages>
<symbols>
<symbol name="RES">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMD-RES-10K-1%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010047</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402FR-0710KL"/>
<attribute name="VALUE" value="10K 1/16W"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-1M-5%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010009</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-071ML"/>
<attribute name="VALUE" value="1M"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-RES-100K-5%-1/16W(0402)" prefix="R" uservalue="yes">
<description>301010033</description>
<gates>
<gate name="G$1" symbol="RES"/>
</gates>
<devices>
<device name="" package="R0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="RC0402JR-07100KL"/>
<attribute name="VALUE" value="100K 1/16W"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-OPL-Diode">
<packages>
<package name="SOD-323">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="DIODE*-1">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMD-DIODE-SCHOTTKY-30V-0.5A(SOD-323)" prefix="D" uservalue="yes">
<description>304020004</description>
<gates>
<gate name="G$1" symbol="DIODE*-1"/>
</gates>
<devices>
<device name="" package="SOD-323">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="LRB551V-30T1G"/>
<attribute name="VALUE" value="30V-0.5A"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SCK_S_v1.0">
<description>Generated from &lt;b&gt;SCK_URBAN_SHIELD_v1.5.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="PINHD_2X8_SMD_FEMALE_UNHOLED">
</package>
<package name="PINHD_2X8_SMD_MALE_UNHOLED">
</package>
</packages>
<symbols>
<symbol name="HANGAR_PINH2X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PINHD_2X8" prefix="JP" uservalue="yes">
<gates>
<gate name="G$1" symbol="HANGAR_PINH2X8"/>
</gates>
<devices>
<device name="FEM_SMD" package="PINHD_2X8_SMD_FEMALE_UNHOLED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MAL_SMD" package="PINHD_2X8_SMD_MALE_UNHOLED">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Seeed-Switch">
<packages>
<package name="SW4-SMD-5.2X5.2X1.5MM">
</package>
</packages>
<symbols>
<symbol name="BOTTON-4P">
<pin name="A0"/>
<pin name="A1"/>
<pin name="B0"/>
<pin name="B1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SMD-BUTTON(4P-5.2X5.2X1.5MM-SKQGADE010)" prefix="SW" uservalue="yes">
<description>311020017</description>
<gates>
<gate name="G$1" symbol="BOTTON-4P"/>
</gates>
<devices>
<device name="-SKQGADE010" package="SW4-SMD-5.2X5.2X1.5MM">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="B0" pad="3"/>
<connect gate="G$1" pin="B1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MPN" value="SKQGADE010"/>
<attribute name="VALUE" value="SKQGADE010"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SCK_BASE_BOARD_v2">
<description>Generated from &lt;b&gt;SCK_BASE_BOARD_v1.5.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="HANGAR_P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="HANGAR_PLCC4_2X2MM">
</package>
</packages>
<symbols>
<symbol name="HANGAR_LED_RGB_CA">
<pin name="A" direction="pas"/>
<pin name="BLUE" direction="pas"/>
<pin name="GREEN" direction="pas"/>
<pin name="RED" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="HANGAR_LED_RGB_CA" prefix="LED">
<description>PLCC-4 RGB LED</description>
<gates>
<gate name="G$1" symbol="HANGAR_LED_RGB_CA"/>
</gates>
<devices>
<device name="ASMB-MTB0-0A3A2" package="HANGAR_P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="BLUE" pad="2"/>
<connect gate="G$1" pin="GREEN" pad="3"/>
<connect gate="G$1" pin="RED" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CLMVC-FKA" package="HANGAR_PLCC4_2X2MM">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="BLUE" pad="2"/>
<connect gate="G$1" pin="GREEN" pad="3"/>
<connect gate="G$1" pin="RED" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ASMB-MTB1-0A3A" package="HANGAR_P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="4"/>
<connect gate="G$1" pin="BLUE" pad="3"/>
<connect gate="G$1" pin="GREEN" pad="2"/>
<connect gate="G$1" pin="RED" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="BAT" library="SparkFun" deviceset="M02" device="-JST-2MM-SMT"/>
<part name="U$23" library="MyPOW" deviceset="VUSB" device=""/>
<part name="GND34" library="supply1" deviceset="GND" device=""/>
<part name="P+11" library="supply1" deviceset="VCC" device=""/>
<part name="P1" library="Hangar" deviceset="SWITCH-MOMENTARY-2" device="KSS"/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="P+18" library="supply1" deviceset="VCC" device=""/>
<part name="GND31" library="SparkFun" deviceset="GND" device=""/>
<part name="GND9" library="SparkFun" deviceset="GND" device=""/>
<part name="P+14" library="supply1" deviceset="VCC" device=""/>
<part name="SD1" library="Hangar" deviceset="SD_CARD_SOCKET" device="TF-01" value="SD_CARD_SOCKETTF-01"/>
<part name="GND25" library="SparkFun" deviceset="GND" device=""/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="GND44" library="supply1" deviceset="GND" device=""/>
<part name="GND51" library="supply1" deviceset="GND" device=""/>
<part name="L3" library="wuerth-elektronik" deviceset="WE-CBF" device="_0402" value="MPZ1005S121C"/>
<part name="L4" library="wuerth-elektronik" deviceset="WE-CBF" device="_0402" value="MPZ1005S121C"/>
<part name="P+17" library="supply1" deviceset="VCC" device=""/>
<part name="F2" library="rcl" deviceset="L-EU" device="L1812" value="MF-MSMF150/12 1500mA"/>
<part name="GND4" library="PowerTags" deviceset="GND" device=""/>
<part name="GND6" library="PowerTags" deviceset="GND" device=""/>
<part name="GND11" library="PowerTags" deviceset="GND" device=""/>
<part name="GND14" library="PowerTags" deviceset="GND" device=""/>
<part name="GND16" library="PowerTags" deviceset="GND" device=""/>
<part name="Y1" library="Cristalli" deviceset="0213_ABS07-32.768KHZ-T" device="" value="32,768Khz"/>
<part name="GND43" library="PowerTags" deviceset="GND" device=""/>
<part name="GND21" library="PowerTags" deviceset="GND" device=""/>
<part name="GND24" library="supply1" deviceset="GND" device=""/>
<part name="GND56" library="supply1" deviceset="GND" device=""/>
<part name="P+3" library="supply1" deviceset="VCC" device=""/>
<part name="P+8" library="supply1" deviceset="VCC" device=""/>
<part name="P+10" library="supply1" deviceset="VCC" device=""/>
<part name="P+13" library="supply1" deviceset="VCC" device=""/>
<part name="P+24" library="supply1" deviceset="VCC" device=""/>
<part name="P+25" library="supply1" deviceset="VCC" device=""/>
<part name="P+1" library="supply1" deviceset="VCC" device=""/>
<part name="P+7" library="supply1" deviceset="VCC" device=""/>
<part name="GND46" library="supply1" deviceset="GND" device=""/>
<part name="GND57" library="supply1" deviceset="GND" device=""/>
<part name="L5" library="wuerth-elektronik" deviceset="WE-CBF" device="_0402" value="MPZ1005S121C"/>
<part name="SWD" library="Hangar" deviceset="PINHEAD_PINHD-2X5" device="SMD" value="20021121-00010C4LF"/>
<part name="P+16" library="supply1" deviceset="VCC" device=""/>
<part name="X1" library="Connector-new" deviceset="GROVE-CONNECTOR-SMD" device="'DD'" value="1125S-SMT-4P"/>
<part name="GND15" library="supply1" deviceset="GND" device=""/>
<part name="FRAME1" library="frames" deviceset="A4L-LOC" device=""/>
<part name="FRAME2" library="frames" deviceset="A4L-LOC" device=""/>
<part name="FRAME3" library="frames" deviceset="A4L-LOC" device=""/>
<part name="IC2" library="SCK_BASE_BOARD_v1.6" deviceset="BQ24259_VQFN(24)" device=""/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="GND17" library="supply1" deviceset="GND" device=""/>
<part name="GND18" library="supply1" deviceset="GND" device=""/>
<part name="GND22" library="supply1" deviceset="GND" device=""/>
<part name="L1" library="SCK_BASE_BOARD_v1.6" deviceset="WUERTH-ELEKTRONIK_WE-CBF" device="_0603" value="BLM18KG101TN1D"/>
<part name="U$2" library="MyPOW" deviceset="VUSB" device=""/>
<part name="GND26" library="supply1" deviceset="GND" device=""/>
<part name="GND28" library="supply1" deviceset="GND" device=""/>
<part name="IC6" library="SCK_BASE_BOARD_v1.6" deviceset="FLASH_S25FL064L" device="" value="UNKNOWN"/>
<part name="P+26" library="supply1" deviceset="VCC" device=""/>
<part name="GND30" library="SparkFun" deviceset="GND" device=""/>
<part name="R1" library="SCK_BASE_BOARD_v1.6" deviceset="HANGAR_R-EU_" device="R0402" value="No BOM"/>
<part name="GND32" library="supply1" deviceset="GND" device=""/>
<part name="GND33" library="supply1" deviceset="GND" device=""/>
<part name="GND35" library="supply1" deviceset="GND" device=""/>
<part name="GND37" library="supply1" deviceset="GND" device=""/>
<part name="GND38" library="supply1" deviceset="GND" device=""/>
<part name="L2" library="SCK_BASE_BOARD_v1.6" deviceset="LQH32PN1R0NNCL" device="" value="1uH"/>
<part name="IC4" library="SCK_BASE_BOARD_v1.6" deviceset="HANGAR_ESP-12-E" device=""/>
<part name="LED3" library="SCK_BASE_BOARD_v1.6" deviceset="LED_SMALL" device="" value="VLMB1500-GS08"/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="GND13" library="supply1" deviceset="GND" device=""/>
<part name="LED2" library="SCK_BASE_BOARD_v1.6" deviceset="LED_SMALL" device="" value="VLMY1500-GS08"/>
<part name="P+2" library="supply1" deviceset="VCC" device=""/>
<part name="GND20" library="supply1" deviceset="GND" device=""/>
<part name="IC5" library="SCK_BASE_BOARD_v1.6" deviceset="HANGAR_SAMD21G18A-" device="MUT" value="SAMD21G18A-MUT"/>
<part name="USB" library="SCK_BASE_BOARD_v1.6" deviceset="HANGAR_MYCON2_USB-MINI-B" device="" value="10118193-0001LF"/>
<part name="F1" library="rcl" deviceset="L-EU" device="L1812" value="MF-MSMF075-2 750mA"/>
<part name="IC3" library="SCK_BASE_BOARD_v1.6" deviceset="LD39200" device=""/>
<part name="P+4" library="supply1" deviceset="VCC" device=""/>
<part name="GND29" library="supply1" deviceset="GND" device=""/>
<part name="GND2" library="SparkFun" deviceset="GND" device=""/>
<part name="Q3" library="SCK_BASE_BOARD_v1.6" deviceset="MOSFETP_BOTH" device="" value="PMOS"/>
<part name="Q4" library="SCK_BASE_BOARD_v1.6" deviceset="MOSFETP_BOTH" device="" value="PMOS"/>
<part name="GND36" library="supply1" deviceset="GND" device=""/>
<part name="R2" library="SCK_URBAN_SHIELD_v1.6" deviceset="HANGAR_R-EU_" device="R0603" value="10mOhm"/>
<part name="GND39" library="supply1" deviceset="GND" device=""/>
<part name="GND40" library="supply1" deviceset="GND" device=""/>
<part name="IC1" library="SCK_URBAN_SHIELD_v1.6" deviceset="GAUGE_BQ2746" device=""/>
<part name="GND41" library="supply1" deviceset="GND" device=""/>
<part name="C4" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-50V-10%-X7R(0805)" device="" value="100nf"/>
<part name="C5" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-10UF-25V-10%-X5R(1206)" device="" value="10uf"/>
<part name="C6" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-1UF-25V-10%-X7R(0805)" device="" value="1uf"/>
<part name="C9" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-47UF-10V-20%-X7R(1210)" device="" value="47uf"/>
<part name="C8" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-10UF-25V-10%-X5R(1206)" device="" value="10uf"/>
<part name="C11" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-1UF-25V-10%-X7R(0805)" device="" value="1uf"/>
<part name="C10" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-50V-10%-X7R(0603)" device="" value="100nf"/>
<part name="R5" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="GND27" library="supply1" deviceset="GND" device=""/>
<part name="GND42" library="supply1" deviceset="GND" device=""/>
<part name="GND45" library="supply1" deviceset="GND" device=""/>
<part name="TVS1" library="fabhack" deviceset="TPD4S012_DRY_6" device=""/>
<part name="C13" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-4.7UF-10V-10%-X5R(0603)" device="" value="4.7uf"/>
<part name="C12" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-4.7UF-10V-10%-X5R(0603)" device="" value="4.7uf"/>
<part name="R9" library="Seeed-OPL-Resistor" deviceset="SMD-RES-100K-5%-1/16W(0402)" device="" value="100K 1/16W"/>
<part name="R10" library="Seeed-OPL-Resistor" deviceset="SMD-RES-47K-5%-1/16W(0402)" device="" value="47K"/>
<part name="R11" library="Seeed-OPL-Resistor" deviceset="SMD-RES-68K-50V-5%(0402)" device="" value="68K"/>
<part name="C17" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-4.7UF-25V-10%-X5R(0805)" device="" value="4.7uf"/>
<part name="C14" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-47NF-25V-10%-X7R(0402)" device="" value="47nf"/>
<part name="C15" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-10UF-10V-10%-X5R(0603)" device="" value="10uf"/>
<part name="C16" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-10UF-10V-10%-X5R(0603)" device="" value="10uf"/>
<part name="R12" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="C18" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-2.2UF-10V-10%-X7R(0603)" device="" value="2.2uf"/>
<part name="C21" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-1UF-25V-10%-X7R(0805)" device="" value="1uf"/>
<part name="C19" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-22PF-50V-5%-NPO(0402)" device="" value="22pf"/>
<part name="C20" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-22PF-50V-5%-NPO(0402)" device="" value="22pf"/>
<part name="R13" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="R14" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="R15" library="Seeed-OPL-Resistor" deviceset="SMD-RES-330R-1%-1/16W(0402)" device="" value="330R"/>
<part name="R16" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="C22" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-25V-10%-X7R(0402)" device="" value="100nf"/>
<part name="C23" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-25V-10%-X7R(0402)" device="" value="100nf"/>
<part name="C24" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-25V-10%-X7R(0402)" device="" value="100nf"/>
<part name="C25" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-25V-10%-X7R(0402)" device="" value="100nf"/>
<part name="C26" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-1UF-10V-10%-X5R(0402)" device="" value="1uf"/>
<part name="R17" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="L6" library="wuerth-elektronik" deviceset="WE-CBF" device="_0402" value="MPZ1005S121C"/>
<part name="SUPPLY1" library="supply2" deviceset="AGND" device=""/>
<part name="R4" library="Seeed-OPL-Resistor" deviceset="SMD-RES-1K-5%-1/16W(0402)" device="" value="1K"/>
<part name="R18" library="Seeed-OPL-Resistor" deviceset="SMD-RES-1K-5%-1/16W(0402)" device="" value="1K"/>
<part name="R19" library="Seeed-OPL-Resistor" deviceset="SMD-RES-1K-5%-1/16W(0402)" device="" value="1K"/>
<part name="R20" library="Seeed-OPL-Resistor" deviceset="SMD-RES-1K-5%-1/16W(0402)" device="" value="1K"/>
<part name="R21" library="Seeed-OPL-Resistor" deviceset="SMD-RES-1K-5%-1/16W(0402)" device="" value="1K"/>
<part name="GND23" library="PowerTags" deviceset="GND" device=""/>
<part name="C3" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-10NF-50V-10%-X7R(0402)" device="" value="10nf"/>
<part name="GND47" library="PowerTags" deviceset="GND" device=""/>
<part name="P+5" library="supply1" deviceset="VCC" device=""/>
<part name="R22" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="R23" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="C1" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-25V-10%-X7R(0402)" device="" value="100nf"/>
<part name="C2" library="Seeed-OPL-Capacitor" deviceset="CERAMIC-100NF-25V-10%-X7R(0402)" device="" value="100nf"/>
<part name="R3" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="R27" library="Seeed-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="GND19" library="supply1" deviceset="GND" device=""/>
<part name="R28" library="Seeed-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="R29" library="Seeed-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="P+12" library="supply1" deviceset="VCC" device=""/>
<part name="P+15" library="supply1" deviceset="VCC" device=""/>
<part name="P+19" library="supply1" deviceset="VCC" device=""/>
<part name="R30" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="D1" library="Seeed-OPL-Diode" deviceset="SMD-DIODE-SCHOTTKY-30V-0.5A(SOD-323)" device="" value="30V-0.5A"/>
<part name="P+20" library="supply1" deviceset="VCC" device=""/>
<part name="Q2" library="SCK_BASE_BOARD_v1.6" deviceset="NMOS_RJU003N03FRAT106" device="" value="NMOS"/>
<part name="P+23" library="supply1" deviceset="VCC" device=""/>
<part name="Q1" library="SCK_BASE_BOARD_v1.6" deviceset="NMOS_RJU003N03FRAT106" device="" value="NMOS"/>
<part name="R38" library="Seeed-Resistor" deviceset="SMD-RES-1M-5%-1/16W(0402)" device="" value="1M"/>
<part name="R39" library="Seeed-Resistor" deviceset="SMD-RES-100K-5%-1/16W(0402)" device="" value="100K 1/16W"/>
<part name="R40" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="P+27" library="supply1" deviceset="VCC" device=""/>
<part name="GND53" library="supply1" deviceset="GND" device=""/>
<part name="P+28" library="supply1" deviceset="VCC" device=""/>
<part name="R43" library="Seeed-Resistor" deviceset="SMD-RES-100K-5%-1/16W(0402)" device="" value="100K 1/16W"/>
<part name="R8" library="Seeed-OPL-Resistor" deviceset="SMD-RES-100K-5%-1/16W(0402)" device="" value="100K 1/16W"/>
<part name="R7" library="Seeed-OPL-Resistor" deviceset="SMD-RES-100K-5%-1/16W(0402)" device="" value="100K 1/16W"/>
<part name="R26" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="GND48" library="supply1" deviceset="GND" device=""/>
<part name="R6" library="Seeed-OPL-Resistor" deviceset="SMD-RES-100K-5%-1/16W(0402)" device="" value="100K 1/16W"/>
<part name="GND49" library="supply1" deviceset="GND" device=""/>
<part name="JP1" library="SCK_S_v1.0" deviceset="PINHD_2X8" device="FEM_SMD"/>
<part name="P2" library="Seeed-Switch" deviceset="SMD-BUTTON(4P-5.2X5.2X1.5MM-SKQGADE010)" device="-SKQGADE010" value="SKQGADE010"/>
<part name="LED1" library="SCK_BASE_BOARD_v2" deviceset="HANGAR_LED_RGB_CA" device="ASMB-MTB1-0A3A"/>
<part name="R24" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
<part name="P+6" library="supply1" deviceset="VCC" device=""/>
<part name="P+9" library="supply1" deviceset="VCC" device=""/>
<part name="R25" library="Seeed-OPL-Resistor" deviceset="SMD-RES-10K-1%-1/16W(0402)" device="" value="10K 1/16W"/>
</parts>
<sheets>
<sheet>
<plain>
<text>FUENTE DC 3.3V</text>
<text>LOW ESR z200mOhm </text>
<text>USB INPUT/OUTPUT</text>
<text>LINEAR REGULATOR </text>
<text>FUEL GAUGE</text>
<text>BATTERY CHARGER &amp; SYSTEM SUPPLY</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="GND12" gate="1" pin="GND"/>
<pinref part="IC3" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND46" gate="1" pin="GND"/>
<pinref part="BAT" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="IC1" gate="BQ27426" pin="VSS"/>
</segment>
<segment>
<pinref part="GND10" gate="1" pin="GND"/>
<pinref part="C17" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="PGND"/>
<pinref part="GND17" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND18" gate="1" pin="GND"/>
<pinref part="IC2" gate="G$1" pin="THERMAL"/>
</segment>
<segment>
<pinref part="GND36" gate="1" pin="GND"/>
<pinref part="C5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND34" gate="1" pin="GND"/>
<pinref part="C6" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND26" gate="1" pin="GND"/>
<pinref part="C13" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND28" gate="1" pin="GND"/>
<pinref part="C12" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND32" gate="1" pin="GND"/>
<pinref part="R11" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND33" gate="1" pin="GND"/>
<pinref part="R1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND35" gate="1" pin="GND"/>
<pinref part="R9" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND37" gate="1" pin="GND"/>
<pinref part="C15" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND38" gate="1" pin="GND"/>
<pinref part="C16" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="USB" gate="G$1" pin="SH1"/>
<pinref part="USB" gate="G$1" pin="SH2"/>
<pinref part="USB" gate="G$1" pin="SH3"/>
<pinref part="USB" gate="G$1" pin="SH4"/>
<pinref part="USB" gate="G$1" pin="SH5"/>
<pinref part="USB" gate="G$1" pin="SH6"/>
<pinref part="USB" gate="G$1" pin="SH7"/>
<pinref part="USB" gate="G$1" pin="SH8"/>
<pinref part="USB" gate="G$1" pin="SH9"/>
<pinref part="USB" gate="G$1" pin="SH10"/>
<pinref part="USB" gate="G$1" pin="SH11"/>
<pinref part="USB" gate="G$1" pin="SH12"/>
<pinref part="USB" gate="G$1" pin="SH13"/>
<pinref part="USB" gate="G$1" pin="SH14"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="USB" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND20" gate="1" pin="GND"/>
<pinref part="IC2" gate="G$1" pin="ILIM"/>
</segment>
<segment>
<pinref part="GND29" gate="1" pin="GND"/>
<pinref part="Q2" gate="G$1" pin="S"/>
</segment>
<segment>
<pinref part="C4" gate="G$1" pin="1"/>
<pinref part="GND27" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND42" gate="1" pin="GND"/>
<pinref part="C11" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND45" gate="1" pin="GND"/>
<pinref part="C10" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="TVS1" gate="A" pin="GND"/>
<pinref part="GND13" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND57" gate="1" pin="GND"/>
<pinref part="C18" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND40" gate="1" pin="GND"/>
<pinref part="C21" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND39" gate="1" pin="GND"/>
<pinref part="R12" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND53" gate="1" pin="GND"/>
<pinref part="R39" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND48" gate="1" pin="GND"/>
<pinref part="R7" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="1"/>
<pinref part="GND49" gate="1" pin="GND"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="P+11" gate="VCC" pin="VCC"/>
<pinref part="F2" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+19" gate="VCC" pin="VCC"/>
<pinref part="R30" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+20" gate="VCC" pin="VCC"/>
<pinref part="R8" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+23" gate="VCC" pin="VCC"/>
<pinref part="R26" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+27" gate="VCC" pin="VCC"/>
<pinref part="R38" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+28" gate="VCC" pin="VCC"/>
<pinref part="R43" gate="G$1" pin="2"/>
</segment>
</net>
<net name="VCC_SOURCE">
<segment>
<pinref part="IC3" gate="G$1" pin="OUT"/>
<pinref part="IC3" gate="G$1" pin="SENSE"/>
<pinref part="F2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="BTST">
<segment>
<pinref part="IC2" gate="G$1" pin="BTST"/>
<pinref part="C14" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VBAT">
<segment>
<pinref part="BAT" gate="G$1" pin="2"/>
<pinref part="R2" gate="G$1" pin="2"/>
<pinref part="IC1" gate="BQ27426" pin="SRP"/>
<pinref part="IC1" gate="BQ27426" pin="BAT"/>
<pinref part="C21" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="IC1" gate="BQ27426" pin="SDA"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="SDA"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="IC1" gate="BQ27426" pin="SCL"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="SCL"/>
</segment>
</net>
<net name="ALARMB">
<segment>
<pinref part="IC1" gate="BQ27426" pin="GPUOT"/>
<pinref part="R43" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SW">
<segment>
<pinref part="IC2" gate="G$1" pin="SW"/>
<pinref part="L2" gate="G$1" pin="1"/>
<pinref part="C14" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$17">
<segment>
<pinref part="IC2" gate="G$1" pin="REGN"/>
<pinref part="R10" gate="G$1" pin="2"/>
<pinref part="C17" gate="G$1" pin="2"/>
</segment>
</net>
<net name="INT_CHG">
<segment>
<pinref part="IC2" gate="G$1" pin="INT"/>
</segment>
<segment>
<pinref part="R30" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VUSB">
<segment>
<pinref part="U$23" gate="G$1" pin="VUSB"/>
<pinref part="L1" gate="G$1" pin="2"/>
<pinref part="C5" gate="G$1" pin="2"/>
<pinref part="C6" gate="G$1" pin="2"/>
<pinref part="C4" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="U$2" gate="G$1" pin="VUSB"/>
<pinref part="IC2" gate="G$1" pin="VBUS"/>
</segment>
</net>
<net name="TARGET_USB_N">
<segment>
<pinref part="USB" gate="G$1" pin="D-"/>
<pinref part="TVS1" gate="A" pin="D-"/>
</segment>
</net>
<net name="TARGET_USB_P">
<segment>
<pinref part="USB" gate="G$1" pin="D+"/>
<pinref part="TVS1" gate="A" pin="D+"/>
</segment>
</net>
<net name="N$19">
<segment>
<pinref part="IC2" gate="G$1" pin="PMID"/>
<pinref part="C12" gate="G$1" pin="2"/>
<pinref part="C13" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$32">
<segment>
<pinref part="IC2" gate="G$1" pin="TS"/>
<pinref part="R1" gate="G$1" pin="2"/>
<pinref part="R10" gate="G$1" pin="1"/>
<pinref part="R11" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$33">
<segment>
<pinref part="IC2" gate="G$1" pin="/CE"/>
<pinref part="R9" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PSEL">
<segment>
<pinref part="IC2" gate="G$1" pin="PSEL"/>
<pinref part="R6" gate="G$1" pin="2"/>
</segment>
</net>
<net name="VSYS">
<segment>
<pinref part="L2" gate="G$1" pin="2"/>
<pinref part="C15" gate="G$1" pin="2"/>
<pinref part="C16" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="IN"/>
<pinref part="R5" gate="G$1" pin="1"/>
<pinref part="C11" gate="G$1" pin="2"/>
<pinref part="C10" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="SYS"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="IC3" gate="G$1" pin="EN"/>
<pinref part="R5" gate="G$1" pin="2"/>
</segment>
</net>
<net name="USB_ID">
<segment>
<pinref part="USB" gate="G$1" pin="ID"/>
<pinref part="TVS1" gate="A" pin="ID"/>
</segment>
<segment>
<pinref part="Q2" gate="G$1" pin="G"/>
<pinref part="R26" gate="G$1" pin="1"/>
<pinref part="R7" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$9">
<segment>
<pinref part="IC1" gate="BQ27426" pin="VDD"/>
<pinref part="C18" gate="G$1" pin="2"/>
</segment>
</net>
<net name="V+1">
<segment>
<pinref part="USB" gate="G$1" pin="VBUS"/>
<pinref part="L1" gate="G$1" pin="1"/>
<pinref part="TVS1" gate="A" pin="VBUS"/>
</segment>
</net>
<net name="VBAT'">
<segment>
<pinref part="R2" gate="G$1" pin="1"/>
<pinref part="IC1" gate="BQ27426" pin="SRN"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="VBAT"/>
</segment>
<segment>
<pinref part="R40" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$14">
<segment>
<pinref part="R12" gate="G$1" pin="2"/>
<pinref part="Q1" gate="G$1" pin="S"/>
</segment>
</net>
<net name="N$20">
<segment>
<pinref part="R39" gate="G$1" pin="2"/>
<pinref part="R40" gate="G$1" pin="1"/>
<pinref part="Q1" gate="G$1" pin="G"/>
</segment>
</net>
<net name="BIN">
<segment>
<pinref part="IC1" gate="BQ27426" pin="BIN"/>
<pinref part="R38" gate="G$1" pin="1"/>
<pinref part="Q1" gate="G$1" pin="D"/>
</segment>
</net>
<net name="OTG">
<segment>
<pinref part="IC2" gate="G$1" pin="OTG"/>
<pinref part="Q2" gate="G$1" pin="D"/>
<pinref part="R8" gate="G$1" pin="1"/>
</segment>
</net>
</nets>
</sheet>
<sheet>
<plain>
<text>PROGRAMADOR USB</text>
<text>Blue</text>
<text>Green</text>
<text>SCL_B</text>
<text>SDA_B</text>
<text>Red</text>
<text>CTRL</text>
<text>SW_G</text>
<text>SW_W</text>
<text>SDA_A</text>
<text>SCL_A</text>
<text>USBLED</text>
<text>TX</text>
<text>RX</text>
<text>D+</text>
<text>D-</text>
<text>RST</text>
<text>SWDIO</text>
<text>SWCLK</text>
<text>PD_Wifi</text>
<text>GPIO0_Wifi</text>
<text>BAT_INS</text>
<text>I2S_SD</text>
<text>HeatCO</text>
<text>Gauge ALM</text>
<text>CHRGR_IRQ</text>
<text>HeatNO</text>
<text>I2S_SD</text>
<text>I2S_FS</text>
<text>SPI_MOSI</text>
<text>SPI_SCK</text>
<text>SPI_MISO</text>
<text>SPI_CS_Flash</text>
<text>SPI_CS_SDcard</text>
<text>CD_SDcard</text>
<text>SW_P</text>
<text>RX_P</text>
<text>TX_P</text>
<text>LED INTERFACE</text>
<text>RESET CONTROL</text>
<text>USER BUTTON</text>
<text>SWD INTERFACE</text>
<text>SAMD21G18 BASIC SYSTEM</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="GND4" gate="1" pin="GND"/>
<pinref part="IC5" gate="G$1" pin="GND1"/>
</segment>
<segment>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="C24" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="IC5" gate="G$1" pin="GND2"/>
<pinref part="GND47" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND11" gate="1" pin="GND"/>
<pinref part="IC5" gate="G$1" pin="GND3"/>
</segment>
<segment>
<pinref part="GND14" gate="1" pin="GND"/>
<pinref part="C26" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND16" gate="1" pin="GND"/>
<pinref part="C25" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND21" gate="1" pin="GND"/>
<pinref part="C23" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND56" gate="1" pin="GND"/>
<pinref part="C3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND22" gate="1" pin="GND"/>
<pinref part="P2" gate="G$1" pin="B1"/>
<pinref part="P2" gate="G$1" pin="B0"/>
</segment>
<segment>
<pinref part="GND24" gate="1" pin="GND"/>
<pinref part="SWD" gate="G$1" pin="3"/>
<pinref part="SWD" gate="G$1" pin="5"/>
<pinref part="SWD" gate="G$1" pin="9"/>
</segment>
<segment>
<pinref part="L6" gate="G$1" pin="1"/>
<pinref part="GND43" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C19" gate="G$1" pin="1"/>
<pinref part="C20" gate="G$1" pin="1"/>
<pinref part="GND23" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="P1" gate="G$1" pin="1"/>
<pinref part="GND5" gate="1" pin="GND"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="IC5" gate="G$1" pin="PA22/I2C/EIC/SCOM5PAD0+/TC4"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="IC5" gate="G$1" pin="PA23/I2C/EIC/SCOM5PAD1+/TC4"/>
</segment>
</net>
<net name="TXLED">
<segment>
<pinref part="IC5" gate="G$1" pin="PA27/EIC"/>
</segment>
<segment>
<pinref part="R18" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="P+18" gate="VCC" pin="VCC"/>
<pinref part="R17" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+3" gate="VCC" pin="VCC"/>
<pinref part="IC5" gate="G$1" pin="VDDIN"/>
<pinref part="C25" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+8" gate="VCC" pin="VCC"/>
<pinref part="IC5" gate="G$1" pin="VDDIO2"/>
<pinref part="C24" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+10" gate="VCC" pin="VCC"/>
<pinref part="L5" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+13" gate="VCC" pin="VCC"/>
<pinref part="IC5" gate="G$1" pin="VDDIO1"/>
<pinref part="C23" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+24" gate="VCC" pin="VCC"/>
<pinref part="R16" gate="G$1" pin="2"/>
<pinref part="D1" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="P+25" gate="VCC" pin="VCC"/>
<pinref part="SWD" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="P+17" gate="VCC" pin="VCC"/>
<pinref part="LED3" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="P+4" gate="VCC" pin="VCC"/>
<pinref part="LED1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="P+2" gate="VCC" pin="VCC"/>
<pinref part="LED2" gate="G$1" pin="A"/>
</segment>
</net>
<net name="CONTROL">
<segment>
<pinref part="R17" gate="G$1" pin="1"/>
<pinref part="P1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="IC5" gate="G$1" pin="PA21/EIC/SCOM5PAD3+"/>
</segment>
</net>
<net name="RESET">
<segment>
<pinref part="R16" gate="G$1" pin="1"/>
<pinref part="R15" gate="G$1" pin="2"/>
<pinref part="D1" gate="G$1" pin="+"/>
<pinref part="P2" gate="G$1" pin="A1"/>
<pinref part="P2" gate="G$1" pin="A0"/>
</segment>
<segment>
<pinref part="SWD" gate="G$1" pin="10"/>
</segment>
</net>
<net name="PA00_XIN32">
<segment>
<pinref part="Y1" gate="G$1" pin="2"/>
<pinref part="IC5" gate="G$1" pin="PA0/XIN32/EIC/SCOM1PAD0/TC2"/>
<pinref part="C19" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PA01_XOUT32">
<segment>
<pinref part="Y1" gate="G$1" pin="1"/>
<pinref part="IC5" gate="G$1" pin="PA1/XOUT32/EIC/SCOM1PAD1/TC2"/>
<pinref part="C20" gate="G$1" pin="2"/>
</segment>
</net>
<net name="TARGET_USB_N">
<segment>
<pinref part="IC5" gate="G$1" pin="PA24/EIC/SCOM3PAD2+/TC5"/>
</segment>
</net>
<net name="TARGET_USB_P">
<segment>
<pinref part="IC5" gate="G$1" pin="PA25/EIC/SCOM3PAD3+/TC5"/>
</segment>
</net>
<net name="VDDCORE">
<segment>
<pinref part="IC5" gate="G$1" pin="VDDCORE1"/>
<pinref part="C26" gate="G$1" pin="2"/>
</segment>
</net>
<net name="PA31_SWDIO">
<segment>
<pinref part="IC5" gate="G$1" pin="PA31/EIC/SCOM1PAD3/TC1"/>
</segment>
<segment>
<pinref part="SWD" gate="G$1" pin="2"/>
</segment>
</net>
<net name="AVCC">
<segment>
<pinref part="L5" gate="G$1" pin="2"/>
<pinref part="IC5" gate="G$1" pin="VDDANA"/>
<pinref part="C22" gate="G$1" pin="2"/>
</segment>
</net>
<net name="TARGET_RESET">
<segment>
<pinref part="IC5" gate="G$1" pin="RESETN"/>
</segment>
<segment>
<pinref part="R15" gate="G$1" pin="1"/>
<pinref part="C3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="IC5" gate="G$1" pin="PB10/EIC/SCOM4PAD2/TC5"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="IC5" gate="G$1" pin="PB11/EIC/SCOM4PAD3/TC5"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="IC5" gate="G$1" pin="PA12/I2C/EIC/SCOM2PAD0+/TC2"/>
</segment>
</net>
<net name="SW_WIFI">
<segment>
<pinref part="IC5" gate="G$1" pin="PB22/EIC/SCOM5PAD2"/>
</segment>
</net>
<net name="CS_MMC">
<segment>
<pinref part="IC5" gate="G$1" pin="PA14/XIN/EIC/SCOM2PAD2+/TC3"/>
</segment>
</net>
<net name="PA30_SWCLK">
<segment>
<pinref part="IC5" gate="G$1" pin="PA30/EIC/SCOM1PAD2/TC1"/>
</segment>
<segment>
<pinref part="SWD" gate="G$1" pin="4"/>
</segment>
</net>
<net name="LED_RED">
<segment>
<pinref part="IC5" gate="G$1" pin="PA20/EIC/SCOM5PAD2+"/>
</segment>
<segment>
<pinref part="R19" gate="G$1" pin="1"/>
</segment>
</net>
<net name="LED_BLUE">
<segment>
<pinref part="IC5" gate="G$1" pin="PA18/EIC/SCOM1PAD2+/TC3"/>
</segment>
<segment>
<pinref part="R21" gate="G$1" pin="1"/>
</segment>
</net>
<net name="LED_GREEN">
<segment>
<pinref part="IC5" gate="G$1" pin="PA19/EIC/SCOM1PAD3+/TC3"/>
</segment>
<segment>
<pinref part="R20" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ALARMB">
<segment>
<pinref part="IC5" gate="G$1" pin="PA2/EIC/AIN0"/>
</segment>
</net>
<net name="I2S_SD">
<segment>
<pinref part="IC5" gate="G$1" pin="PA7/EIC/AIN7/SCOM0PAD3/TC1"/>
</segment>
</net>
<net name="INT_CHG">
<segment>
<pinref part="IC5" gate="G$1" pin="PA3/EIC/REF/AIN1"/>
</segment>
</net>
<net name="I2S_SCK">
<segment>
<pinref part="IC5" gate="G$1" pin="PA10/EIC/AIN18/SCOM2PAD2+/TC1"/>
</segment>
</net>
<net name="I2S_FS">
<segment>
<pinref part="IC5" gate="G$1" pin="PA11/EIC/AIN19/SCOM2PAD3+/TC1"/>
</segment>
</net>
<net name="CD_MMC">
<segment>
<pinref part="IC5" gate="G$1" pin="PA15/XOUT/EIC/SCOM2PAD3+/TC3"/>
</segment>
</net>
<net name="SDA_GROOVE">
<segment>
<pinref part="IC5" gate="G$1" pin="PA16/I2C/EIC/SCOM1PAD0+/TC2"/>
</segment>
</net>
<net name="SCL_GROOVE">
<segment>
<pinref part="IC5" gate="G$1" pin="PA17/I2C/EIC/SCOM1PAD1+/TC2"/>
</segment>
</net>
<net name="SW_GROOVE">
<segment>
<pinref part="IC5" gate="G$1" pin="PB23/EIC/SCOM5PAD3"/>
</segment>
</net>
<net name="CS_FLASH">
<segment>
<pinref part="IC5" gate="G$1" pin="PA13/I2C/EIC/SCOM2PAD1+/TC2"/>
</segment>
</net>
<net name="CH_PD">
<segment>
<pinref part="IC5" gate="G$1" pin="PB8/EIC/AIN2/SCOM4PAD0/TC4"/>
</segment>
</net>
<net name="GPIO0">
<segment>
<pinref part="IC5" gate="G$1" pin="PB9/EIC/AIN3/SCOM4PAD1//TC4"/>
</segment>
</net>
<net name="PWM_HEATER_NOX">
<segment>
<pinref part="IC5" gate="G$1" pin="PA9/I2C/EIC/AIN17/SCOM2PAD1+/TC0"/>
</segment>
</net>
<net name="PWM_HEATER_CO">
<segment>
<pinref part="IC5" gate="G$1" pin="PA8/I2C/AIN16/SCOM2PAD0+/TC0"/>
</segment>
</net>
<net name="RXWIFI">
<segment>
<pinref part="IC5" gate="G$1" pin="PA5/EIC/AIN5/SCOM0PAD1/TC0"/>
</segment>
</net>
<net name="TXWIFI">
<segment>
<pinref part="IC5" gate="G$1" pin="PA4/EIC/REF/AIN4/SCOM0PAD0/TC0"/>
</segment>
</net>
<net name="WIFI_LED">
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="LED3" gate="G$1" pin="K"/>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="R20" gate="G$1" pin="2"/>
<pinref part="LED1" gate="G$1" pin="GREEN"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="R19" gate="G$1" pin="2"/>
<pinref part="LED1" gate="G$1" pin="RED"/>
</segment>
</net>
<net name="N$11">
<segment>
<pinref part="R21" gate="G$1" pin="2"/>
<pinref part="LED1" gate="G$1" pin="BLUE"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="LED2" gate="G$1" pin="K"/>
<pinref part="R18" gate="G$1" pin="2"/>
</segment>
</net>
<net name="AGND">
<segment>
<pinref part="IC5" gate="G$1" pin="GNDANA"/>
<pinref part="SUPPLY1" gate="G$1" pin="AGND"/>
<pinref part="L6" gate="G$1" pin="2"/>
<pinref part="C22" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SW_PMS">
<segment>
<pinref part="IC5" gate="G$1" pin="PA28/EIC"/>
</segment>
</net>
<net name="RX_PMS">
<segment>
<pinref part="IC5" gate="G$1" pin="PB3/EIC/AIN11/SCOM5PAD1"/>
</segment>
</net>
<net name="TX_PMS">
<segment>
<pinref part="IC5" gate="G$1" pin="PB2/EIC/AIN10/SCOM5PAD0"/>
</segment>
</net>
<net name="BIN">
<segment>
<pinref part="IC5" gate="G$1" pin="PA6/EIC/AIN6/SCOM0PAD2/TC1"/>
</segment>
</net>
</nets>
</sheet>
<sheet>
<plain>
<text>MODULO INALAMBRICO</text>
<text>SD CARD</text>
<text>Winbond</text>
<text>URBAN SHIELD PORT</text>
<text>GROOVE PORT</text>
<text>MICRO SD CARD SOCKET</text>
<text>ESP8266 MODULE</text>
<text>EXTERNAL FLASH MEMORY</text>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="GND31" gate="1" pin="GND"/>
<pinref part="SD1" gate="G$1" pin="SWITCH_B"/>
<pinref part="SD1" gate="G$1" pin="SHIELD"/>
</segment>
<segment>
<pinref part="GND9" gate="1" pin="GND"/>
<pinref part="SD1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND30" gate="1" pin="GND"/>
<pinref part="IC6" gate="G$1" pin="VSS"/>
</segment>
<segment>
<pinref part="L4" gate="G$1" pin="2"/>
<pinref part="GND25" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="C2" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND51" gate="1" pin="GND"/>
<pinref part="JP1" gate="G$1" pin="14"/>
<pinref part="JP1" gate="G$1" pin="16"/>
</segment>
<segment>
<pinref part="GND15" gate="1" pin="GND"/>
<pinref part="X1" gate="G$1" pin="SS2"/>
<pinref part="X1" gate="G$1" pin="4"/>
<pinref part="X1" gate="G$1" pin="SS1"/>
</segment>
<segment>
<pinref part="GND19" gate="1" pin="GND"/>
<pinref part="JP1" gate="G$1" pin="15"/>
</segment>
<segment>
<pinref part="GND44" gate="1" pin="GND"/>
<pinref part="C9" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND41" gate="1" pin="GND"/>
<pinref part="C8" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R27" gate="G$1" pin="1"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
</net>
<net name="TXWIFI">
<segment>
<pinref part="IC4" gate="G$1" pin="RXD"/>
</segment>
</net>
<net name="RXWIFI">
<segment>
<pinref part="IC4" gate="G$1" pin="TXD"/>
</segment>
</net>
<net name="CH_PD">
<segment>
<pinref part="IC4" gate="G$1" pin="CH_PD"/>
</segment>
</net>
<net name="GPIO0">
<segment>
<pinref part="IC4" gate="G$1" pin="GPIO0"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="P+14" gate="VCC" pin="VCC"/>
<pinref part="SD1" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="VCC"/>
<pinref part="P+26" gate="VCC" pin="VCC"/>
<pinref part="C2" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+1" gate="VCC" pin="VCC"/>
<pinref part="R13" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+7" gate="VCC" pin="VCC"/>
<pinref part="R14" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+5" gate="VCC" pin="VCC"/>
<pinref part="JP1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="P+16" gate="VCC" pin="VCC"/>
<pinref part="JP1" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="F1" gate="G$1" pin="2"/>
<pinref part="P+12" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="Q4" gate="G$1" pin="S"/>
<pinref part="Q4" gate="G$2" pin="S"/>
<pinref part="C9" gate="G$1" pin="2"/>
<pinref part="R28" gate="G$1" pin="2"/>
<pinref part="P+15" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="R24" gate="G$1" pin="2"/>
<pinref part="P+6" gate="VCC" pin="VCC"/>
</segment>
<segment>
<pinref part="R25" gate="G$1" pin="2"/>
<pinref part="P+9" gate="VCC" pin="VCC"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="SD1" gate="G$1" pin="DI/CMD"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="SI/IO0"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="SD1" gate="G$1" pin="CLK"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="SCK"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="SD1" gate="G$1" pin="DO/DAT0"/>
</segment>
<segment>
<pinref part="IC6" gate="G$1" pin="SO/IO1"/>
</segment>
</net>
<net name="CS_MMC">
<segment>
<pinref part="SD1" gate="G$1" pin="CS/DAT3"/>
<pinref part="R25" gate="G$1" pin="1"/>
</segment>
</net>
<net name="GND_WIFI">
<segment>
<pinref part="L4" gate="G$1" pin="1"/>
<pinref part="IC4" gate="G$1" pin="GND"/>
<pinref part="IC4" gate="G$1" pin="GPIO15"/>
<pinref part="IC4" gate="G$1" pin="GPIO4"/>
<pinref part="C1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="WIFI_LED">
<segment>
<pinref part="IC4" gate="G$1" pin="GPIO5"/>
</segment>
</net>
<net name="RESET">
<segment>
<pinref part="IC4" gate="G$1" pin="GPIO14"/>
</segment>
</net>
<net name="CS_FLASH">
<segment>
<pinref part="IC6" gate="G$1" pin="CS#"/>
<pinref part="R24" gate="G$1" pin="1"/>
</segment>
</net>
<net name="VCC_WIFI">
<segment>
<pinref part="IC4" gate="G$1" pin="GPIO2"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="2"/>
<pinref part="L3" gate="G$1" pin="1"/>
<pinref part="IC4" gate="G$1" pin="RESET"/>
<pinref part="IC4" gate="G$1" pin="VCC"/>
<pinref part="C1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="IC4" gate="G$1" pin="CS0"/>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
</net>
<net name="CD_MMC">
<segment>
<pinref part="SD1" gate="G$1" pin="SWITCH_A"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="R13" gate="G$1" pin="1"/>
<pinref part="JP1" gate="G$1" pin="6"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="R14" gate="G$1" pin="1"/>
<pinref part="JP1" gate="G$1" pin="4"/>
</segment>
</net>
<net name="I2S_SD">
<segment>
<pinref part="JP1" gate="G$1" pin="10"/>
</segment>
</net>
<net name="I2S_SCK">
<segment>
<pinref part="JP1" gate="G$1" pin="8"/>
</segment>
</net>
<net name="I2S_FS">
<segment>
<pinref part="JP1" gate="G$1" pin="12"/>
</segment>
</net>
<net name="PWM_HEATER_NOX">
<segment>
<pinref part="JP1" gate="G$1" pin="3"/>
</segment>
</net>
<net name="PWM_HEATER_CO">
<segment>
<pinref part="JP1" gate="G$1" pin="5"/>
</segment>
</net>
<net name="VCC_GROOVE">
<segment>
<pinref part="X1" gate="G$1" pin="3"/>
<pinref part="R22" gate="G$1" pin="2"/>
<pinref part="R23" gate="G$1" pin="2"/>
<pinref part="Q3" gate="G$1" pin="D"/>
<pinref part="Q3" gate="G$2" pin="D"/>
</segment>
</net>
<net name="SDA_GROOVE">
<segment>
<pinref part="X1" gate="G$1" pin="2"/>
<pinref part="R23" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SCL_GROOVE">
<segment>
<pinref part="X1" gate="G$1" pin="1"/>
<pinref part="R22" gate="G$1" pin="1"/>
</segment>
</net>
<net name="RX_PMS">
<segment>
<pinref part="JP1" gate="G$1" pin="11"/>
</segment>
</net>
<net name="TX_PMS">
<segment>
<pinref part="JP1" gate="G$1" pin="13"/>
</segment>
</net>
<net name="VCC_GROOVE_0">
<segment>
<pinref part="F1" gate="G$1" pin="1"/>
<pinref part="C8" gate="G$1" pin="2"/>
<pinref part="R29" gate="G$1" pin="1"/>
<pinref part="Q3" gate="G$2" pin="S"/>
<pinref part="Q3" gate="G$1" pin="S"/>
</segment>
</net>
<net name="SW_GROOVE">
<segment>
<pinref part="Q3" gate="G$1" pin="G"/>
<pinref part="Q3" gate="G$2" pin="G"/>
<pinref part="R29" gate="G$1" pin="2"/>
</segment>
</net>
<net name="SW_WIFI">
<segment>
<pinref part="Q4" gate="G$1" pin="G"/>
<pinref part="Q4" gate="G$2" pin="G"/>
<pinref part="R28" gate="G$1" pin="1"/>
</segment>
</net>
<net name="SW_PMS">
<segment>
<pinref part="R27" gate="G$1" pin="2"/>
<pinref part="JP1" gate="G$1" pin="7"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="L3" gate="G$1" pin="2"/>
<pinref part="Q4" gate="G$1" pin="D"/>
<pinref part="Q4" gate="G$2" pin="D"/>
</segment>
</net>
<net name="VBAT'">
<segment>
<pinref part="JP1" gate="G$1" pin="9"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
